IFC building model
Schema: "IFC2X3"
Description: "IFC2x3 Coordination View"
File name: "C:\BoligProdusentenes forening\DDS\Blueberry081203_mm\Blueberry081203_mm.ifc"
Time stamp: "2008-12-04T11:25:41"
Author: "Leif Johnsen"
Organization: "Systemair AS"
Preprocessor: "Eurostep IFC Toolbox - 1.0"
Originating system: "AutoCAD Architecture 2009 Build 5.7.68.0"
Application: "AutoCAD Architecture 2009" version "5.7.68.0" identifier "7004" by Organization "Systemair AS"

People and organizations
  Person (no name given) of Organization "Systemair AS"
  Owner history of Person (no name given) of Organization "Systemair AS" | application "AutoCAD Architecture 2009" version "5.7.68.0" identifier "7004" by Organization "Systemair AS" | change NOCHANGE | created 1228386332 (2008-12-04T10:25:32Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: MILLI SQUARE_METRE
  VOLUMEUNIT: MILLI CUBIC_METRE
  PLANEANGLEUNIT: degree (conversion based)
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT "DDS Project" | long name "Blueberry081203_mm"
  IFCSITE "Site" | elevation above sea level -999. | postal address (none given)
    contains 1 element
      1 x IFCBUILDINGELEMENTPROXY
    IFCBUILDING "Blueberry081203_mm" | postal address (none given)
      IFCBUILDINGSTOREY "2" | elevation 2713.99998664856 | description "2"
        contains 69 elements
          8 x IFCWALL | type IFCWALLTYPE "IFCSTYLE (1)" | names: "WALL | IFCSTYLE (1)(1)", "WALL | IFCSTYLE (1)(2)", "WALL | IFCSTYLE (1)(3)" (+5 more) | descriptions: "148 mm bindingsverk, liggende m dobbeltfals" | property sets: Pset_WallCommon, Pset_ADT_Wall, Wall quantities
          4 x IFCWINDOW | type IFCWINDOWSTYLE "D-51-1000-1400" | names: "WINDOW | D-51-1000-1400(1)", "WINDOW | D-51-1000-1400(2)", "WINDOW | D-51-1000-1400(3)" (+1 more) | descriptions: "51: Lukke 2 fag T-spross 1/3 høyde" | property sets: Pset_WindowCommon
          6 x IFCDOOR | type IFCDOORSTYLE "D-16-900-2100" | names: "DOOR | D-16-900-2100(1)", "DOOR | D-16-900-2100(2)", "DOOR | D-16-900-2100(3)" (+3 more) | descriptions: "16: Balkongdør", "0: Standard innerdør", "30: Kottdør" | property sets: Pset_DoorCommon, Pset_ADT_Door
          6 x IFCWALL | type IFCWALLTYPE "IFCSTYLE (2)" | names: "WALL | IFCSTYLE (2)(1)", "WALL | IFCSTYLE (2)(2)", "WALL | IFCSTYLE (2)(3)" (+3 more) | descriptions: "68 mm bindingsverk, innervegg" | property sets: Pset_WallCommon, Pset_ADT_Wall, Wall quantities
          6 x IFCWALL | type IFCWALLTYPE "IFCSTYLE (3)" | names: "WALL | IFCSTYLE (3)(1)", "WALL | IFCSTYLE (3)(2)", "WALL | IFCSTYLE (3)(3)" (+3 more) | descriptions: "98 mm bindingsverk, innervegg" | property sets: Pset_WallCommon, Pset_ADT_Wall, Wall quantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IFCSTYLE (4)" | names: "WALL | IFCSTYLE (4)(1)", "WALL | IFCSTYLE (4)(2)", "WALL | IFCSTYLE (4)(3)" | descriptions: "68 mm balkongrekke" | material: layers "IFCSTYLE (4)" ("68 mm enkelt bindingsverk heltre impregnert" 86.99999749660492) | property sets: Pset_WallCommon, Pset_ADT_Wall, Wall quantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor-100" | names: "SLAB | Floor-100(1)" | descriptions: "Floor-1-100" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor-100 (2)" | names: "SLAB | Floor-100 (2)(1)" | descriptions: "Floor-1-100" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor-100 (3)" | names: "SLAB | Floor-100 (3)(1)" | descriptions: "Floor-1-100" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor-100 (4)" | names: "SLAB | Floor-100 (4)(1)" | descriptions: "Floor-1-100" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor-100 (5)" | names: "SLAB | Floor-100 (5)(1)" | descriptions: "Floor-1-100" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor-14" | names: "SLAB | Floor-14(1)" | descriptions: "Etasjeskille 250 mm I-bjelke" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor-20" | names: "SLAB | Floor-20(1)" | descriptions: "Balkonggulv 148 mm" | material: layers "Floor-20" ("22 mm terrassebord" 21.99999988079071, "148 mm bjelke" 148.0000019073486) | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (0)" | ROOF | names: "ROOFSLAB | IFCSTYLE (0)(1)" | descriptions: "Roof-1-40.00" | material: layers "IFCSTYLE (0)" ("12mm taktro" 12.00000010430813, "48mm lekt/luftespalte" 48.00000041723251, "2mm vindsperre" 2.000000094994903, "198mm taksperr og isolasjon" 197.9999989271164) | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (1)" | ROOF | names: "ROOFSLAB | IFCSTYLE (1)(1)" | descriptions: "Roof-1-40.00" | material: layers "IFCSTYLE (1)" ("12mm taktro" 12.00000010430813, "48mm lekt/luftespalte" 48.00000041723251, "2mm vindsperre" 2.000000094994903, "198mm taksperr og isolasjon" 197.9999989271164) | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (2)" | ROOF | names: "ROOFSLAB | IFCSTYLE (2)(1)" | descriptions: "Roof-1-40.00" | material: layers "IFCSTYLE (2)" ("12mm taktro" 12.00000010430813, "48mm lekt/luftespalte" 48.00000041723251, "2mm vindsperre" 2.000000094994903, "198mm taksperr og isolasjon" 197.9999989271164) | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (3)" | ROOF | names: "ROOFSLAB | IFCSTYLE (3)(1)" | descriptions: "Roof-1-40.00" | material: layers "IFCSTYLE (3)" ("12mm taktro" 12.00000010430813, "48mm lekt/luftespalte" 48.00000041723251, "2mm vindsperre" 2.000000094994903, "198mm taksperr og isolasjon" 197.9999989271164) | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (4)" | ROOF | names: "ROOFSLAB | IFCSTYLE (4)(1)" | descriptions: "Roof-3-40.00" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (5)" | ROOF | names: "ROOFSLAB | IFCSTYLE (5)(1)" | descriptions: "Roof-3-40.00" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (6)" | ROOF | names: "ROOFSLAB | IFCSTYLE (6)(1)" | descriptions: "Roof-3-40.00" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (7)" | ROOF | names: "ROOFSLAB | IFCSTYLE (7)(1)" | descriptions: "Roof-3-40.00" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (8)" | ROOF | names: "ROOFSLAB | IFCSTYLE (8)(1)" | descriptions: "Roof-2-0.00" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (9)" | ROOF | names: "ROOFSLAB | IFCSTYLE (9)(1)" | descriptions: "Roof-2-0.00" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (10)" | ROOF | names: "ROOFSLAB | IFCSTYLE (10)(1)" | descriptions: "Roof-2-40.00" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (11)" | ROOF | names: "ROOFSLAB | IFCSTYLE (11)(1)" | descriptions: "Roof-2-40.00" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (12)" | ROOF | names: "ROOFSLAB | IFCSTYLE (12)(1)" | descriptions: "Roof-2-40.00" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (13)" | ROOF | names: "ROOFSLAB | IFCSTYLE (13)(1)" | descriptions: "Roof-2-40.00" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (14)" | ROOF | names: "ROOFSLAB | IFCSTYLE (14)(1)" | descriptions: "Roof-2-40.00" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCBEAM | type IFCBEAMTYPE "IFCSTYLE (1)" | names: "BEAM | IFCSTYLE (1)(1)" | descriptions: "Beam-2" | property sets: Beam-2
          1 x IFCBEAM | type IFCBEAMTYPE "IFCSTYLE (2)" | names: "BEAM | IFCSTYLE (2)(1)" | descriptions: "Beam-2" | property sets: Beam-2
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "IFCSTYLE (3)" | names: "COLUMN | IFCSTYLE (3)(1)" | descriptions: "Column-2" | property sets: Column-2
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "IFCSTYLE (4)" | names: "COLUMN | IFCSTYLE (4)(1)" | descriptions: "Column-2" | property sets: Column-2
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "IFCSTYLE (5)" | names: "COLUMN | IFCSTYLE (5)(1)" | descriptions: "Column-2" | property sets: Column-2
          9 x IFCBUILDINGELEMENTPROXY | names: "BUILDINGELEMENTPROXY(1)", "BUILDINGELEMENTPROXY(2)", "BUILDINGELEMENTPROXY(3)" (+6 more)
        IFCSPACE "2-1" | long name "Soverom 1" | object type "IFCSTYLE" | description "Soverom 1"
        IFCSPACE "2-2" | long name "Soverom 2" | object type "IFCSTYLE" | description "Soverom 2"
        IFCSPACE "2-3" | long name "Soverom 3" | object type "IFCSTYLE" | description "Soverom 3"
        IFCSPACE "2-4" | long name "Bad" | object type "IFCSTYLE" | description "Bad"
        IFCSPACE "2-5" | long name "Kott" | object type "IFCSTYLE" | description "Kott"
        IFCSPACE "2-6" | long name "Loftstue" | object type "IFCSTYLE" | description "Loftstue"
      IFCBUILDINGSTOREY "1" | elevation 0. | description "1"
        contains 82 elements
          11 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IFCSTYLE (1)" | names: "WALL | IFCSTYLE (1)(1)", "WALL | IFCSTYLE (1)(2)", "WALL | IFCSTYLE (1)(3)" (+8 more) | descriptions: "148 mm bindingsverk, liggende m dobbeltfals" | material: layers "IFCSTYLE (1)" ("19 mm liggende, utvendig panel m/dobbelfals" 18.99999938905239, "23 mm utlekting på fasade c/c 60" 23.00000004470348, "12 mm asfaltimpregnert trefiberplate" 12.00000010430813, "148 mm enkelt bindingsverk heltre isolert" 148.0000019073486, "13 mm gipsplate innvendig kledning" 13.0000002682209) | property sets: Pset_WallCommon, Pset_ADT_Wall, Wall quantities
          6 x IFCWINDOW | type IFCWINDOWSTYLE "D-33-1100-1700" | names: "WINDOW | D-33-1100-1700(1)", "WINDOW | D-33-1100-1700(2)", "WINDOW | D-33-1100-1700(3)" (+3 more) | descriptions: "33: Fast 2 fag T-spross 1/3 høyde", "34: Fast 3 fag T-spross 1/3 høyde", "51: Lukke 2 fag T-spross 1/3 høyde" | property sets: Pset_WindowCommon
          6 x IFCDOOR | type IFCDOORSTYLE "D-336-1000-2100" | names: "DOOR | D-336-1000-2100(1)", "DOOR | D-336-1000-2100(2)", "DOOR | D-336-1000-2100(3)" (+3 more) | descriptions: "336: Puccini M72", "16: Balkongdør", "0: Standard innerdør" | property sets: Pset_DoorCommon, Pset_ADT_Door
          3 x IFCWALL | type IFCWALLTYPE "IFCSTYLE (1)" | names: "WALL | IFCSTYLE (1)(8)", "WALL | IFCSTYLE (1)(9)", "WALL | IFCSTYLE (1)(10)" | descriptions: "148 mm bindingsverk, liggende m dobbeltfals" | material: layers "IFCSTYLE (1)" ("19 mm liggende, utvendig panel m/dobbelfals" 18.99999938905239, "23 mm utlekting på fasade c/c 60" 23.00000004470348, "12 mm asfaltimpregnert trefiberplate" 12.00000010430813, "148 mm enkelt bindingsverk heltre isolert" 148.0000019073486, "13 mm gipsplate innvendig kledning" 13.0000002682209) | property sets: Pset_WallCommon, Pset_ADT_Wall, Wall quantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IFCSTYLE (2)" | names: "WALL | IFCSTYLE (2)(1)", "WALL | IFCSTYLE (2)(2)" | descriptions: "98 mm bindingsverk, innervegg" | material: layers "IFCSTYLE (2)" ("13 mm gipsplate innvendig kledning" 13.0000002682209, "98 mm enkelt bindingsverk heltre" 97.99999743700028, "13 mm gipsplate innvendig kledning" 13.0000002682209) | property sets: Pset_WallCommon, Pset_ADT_Wall, Wall quantities
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IFCSTYLE (3)" | names: "WALL | IFCSTYLE (3)(1)", "WALL | IFCSTYLE (3)(2)", "WALL | IFCSTYLE (3)(3)" (+2 more) | descriptions: "68 mm bindingsverk, innervegg" | material: layers "IFCSTYLE (3)" ("12 mm spon" 13.0000002682209, "68 mm enkelt bindingsverk heltre" 68.00000369548798, "12 mm spon" 13.0000002682209) | property sets: Pset_WallCommon, Pset_ADT_Wall, Wall quantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IFCSTYLE (4)" | names: "WALL | IFCSTYLE (4)(1)" | descriptions: "108 mm pusset tegl" | material: layers "IFCSTYLE (4)" ("10 mm puss" 9.999999776482582, "108 mm tegl" 108.0000028014183, "10 mm puss" 9.999999776482582) | property sets: Pset_WallCommon, Pset_ADT_Wall, Wall quantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IFCSTYLE (5)" | names: "WALL | IFCSTYLE (5)(1)", "WALL | IFCSTYLE (5)(2)", "WALL | IFCSTYLE (5)(3)" (+1 more) | descriptions: "68 mm balkongrekke" | material: layers "IFCSTYLE (5)" ("68 mm enkelt bindingsverk heltre impregnert" 86.99999749660492) | property sets: Pset_WallCommon, Pset_ADT_Wall, Wall quantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor-14" | names: "SLAB | Floor-14(1)" | descriptions: "Etasjeskille 250 mm I-bjelke" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (0)" | ROOF | names: "ROOFSLAB | IFCSTYLE (0)(1)" | descriptions: "Roof-1-40.00" | material: layers "IFCSTYLE (0)" ("12mm taktro" 12.00000010430813, "48mm lekt/luftespalte" 48.00000041723251, "2mm vindsperre" 2.000000094994903, "198mm taksperr og isolasjon" 197.9999989271164) | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (1)" | ROOF | names: "ROOFSLAB | IFCSTYLE (1)(1)" | descriptions: "Roof-3-40.00" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (2)" | ROOF | names: "ROOFSLAB | IFCSTYLE (2)(1)" | descriptions: "Roof-2-40.00" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCSLAB | type IFCSLABTYPE "IFCSTYLE (3)" | ROOF | names: "ROOFSLAB | IFCSTYLE (3)(1)" | descriptions: "Roof-2-0.00" | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          1 x IFCBEAM | type IFCBEAMTYPE "IFCSTYLE (1)" | names: "BEAM | IFCSTYLE (1)(1)" | descriptions: "Beam-2" | property sets: Beam-2
          1 x IFCBEAM | type IFCBEAMTYPE "IFCSTYLE (2)" | names: "BEAM | IFCSTYLE (2)(1)" | descriptions: "Beam-2" | property sets: Beam-2
          1 x IFCBEAM | type IFCBEAMTYPE "IFCSTYLE (3)" | names: "BEAM | IFCSTYLE (3)(1)" | descriptions: "Beam-2" | property sets: Beam-2
          1 x IFCBEAM | type IFCBEAMTYPE "IFCSTYLE (4)" | names: "BEAM | IFCSTYLE (4)(1)" | descriptions: "Beam-2" | property sets: Beam-2
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "IFCSTYLE (5)" | names: "COLUMN | IFCSTYLE (5)(1)" | descriptions: "Column-2" | property sets: Column-2
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "IFCSTYLE (6)" | names: "COLUMN | IFCSTYLE (6)(1)" | descriptions: "Column-2" | property sets: Column-2
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "IFCSTYLE (7)" | names: "COLUMN | IFCSTYLE (7)(1)" | descriptions: "Column-2" | property sets: Column-2
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "IFCSTYLE (8)" | names: "COLUMN | IFCSTYLE (8)(1)" | descriptions: "Column-2" | property sets: Column-2
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "IFCSTYLE (9)" | names: "COLUMN | IFCSTYLE (9)(1)" | descriptions: "Column-2" | property sets: Column-2
          30 x IFCBUILDINGELEMENTPROXY | names: "BUILDINGELEMENTPROXY(1)", "BUILDINGELEMENTPROXY(2)", "BUILDINGELEMENTPROXY(3)" (+27 more)
        IFCSPACE "1-1" | long name "Stue/trapp" | object type "IFCSTYLE" | description "Stue/trapp"
        IFCSPACE "1-2" | long name "Kjøkken" | object type "IFCSTYLE" | description "Kjøkken"
        IFCSPACE "1-3" | long name "Entre" | object type "IFCSTYLE" | description "Entre"
        IFCSPACE "1-4" | long name "Vaskerom" | object type "IFCSTYLE" | description "Vaskerom"
        IFCSPACE "1-5" | long name "WC" | object type "IFCSTYLE" | description "WC"
      IFCBUILDINGSTOREY "0" | elevation -2713.99998664856 | description "0"
        contains 42 elements
          12 x IFCWALL | type IFCWALLTYPE "IFCSTYLE (1)" | names: "WALL | IFCSTYLE (1)(1)", "WALL | IFCSTYLE (1)(2)", "WALL | IFCSTYLE (1)(3)" (+9 more) | descriptions: "200 mm betong" | parts: 2 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, Pset_ADT_Wall, Wall quantities
          4 x IFCWINDOW | type IFCWINDOWSTYLE "D-11-1000-400" | names: "WINDOW | D-11-1000-400(1)", "WINDOW | D-11-1000-400(2)", "WINDOW | D-11-1000-400(3)" (+1 more) | descriptions: "11: Lukke" | property sets: Pset_WindowCommon
          15 x IFCWALL | type IFCWALLTYPE "IFCSTYLE (2)" | names: "WALL | IFCSTYLE (2)(1)", "WALL | IFCSTYLE (2)(2)", "WALL | IFCSTYLE (2)(3)" (+12 more) | descriptions: "68(98) mm påforingsvegg" | parts: 8 IFCBUILDINGELEMENTPART | property sets: Pset_WallCommon, Pset_ADT_Wall, Wall quantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IFCSTYLE (3)" | names: "WALL | IFCSTYLE (3)(1)", "WALL | IFCSTYLE (3)(2)" | descriptions: "150 mm betong" | material: layers "IFCSTYLE (3)" ("150 mm betong" 150.0000059604645) | property sets: Pset_WallCommon, Pset_ADT_Wall, Wall quantities
          3 x IFCDOOR | type IFCDOORSTYLE "D-0-900-2100" | names: "DOOR | D-0-900-2100(1)", "DOOR | D-0-900-2100(2)", "DOOR | D-0-900-2100(3)" | descriptions: "0: Standard innerdør" | property sets: Pset_DoorCommon, Pset_ADT_Door
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IFCSTYLE (4)" | names: "WALL | IFCSTYLE (4)(1)" | descriptions: "68 mm påforingsvegg" | material: layers "IFCSTYLE (4)" ("68 mm enkelt bindingsverk heltre isolert" 68.00000369548798, "13 mm gipsplate innvendig kledning" 13.0000002682209) | property sets: Pset_WallCommon, Pset_ADT_Wall, Wall quantities
          1 x IFCWALL | type IFCWALLTYPE "IFCSTYLE (4)" | names: "WALL | IFCSTYLE (4)(2)" | descriptions: "68 mm påforingsvegg" | parts: 2 IFCBUILDINGELEMENTPART | material: layers "IFCSTYLE (4)" ("68 mm enkelt bindingsverk heltre isolert" 68.00000369548798, "13 mm gipsplate innvendig kledning" 13.0000002682209) | property sets: Pset_WallCommon, Pset_ADT_Wall, Wall quantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IFCSTYLE (5)" | names: "WALL | IFCSTYLE (5)(1)" | descriptions: "68 mm bindingsverk, innervegg isolert" | material: layers "IFCSTYLE (5)" ("12 mm spon" 13.0000002682209, "68 mm enkelt bindingsverk heltre isolert" 68.00000369548798, "12 mm spon" 13.0000002682209) | property sets: Pset_WallCommon, Pset_ADT_Wall, Wall quantities
          1 x IFCSLAB | type IFCSLABTYPE "Floor-31" | names: "SLAB | Floor-31(1)" | descriptions: "Golv på grunn" | material: layers "Floor-31" ("50 mm betong" 50.00000074505806, "50 mm isolasjon" 50.00000074505806, "150 mm isolasjon" 150.0000059604645) | property sets: Pset_SlabCommon, Pset_ADT_Slab, Slab quantities
          2 x IFCBUILDINGELEMENTPROXY | names: "BUILDINGELEMENTPROXY(1)", "BUILDINGELEMENTPROXY(2)"
        IFCSPACE "0-1" | long name "Disponibelt" | object type "IFCSTYLE" | description "Disponibelt"
        IFCSPACE "0-2" | long name "Diverse" | object type "IFCSTYLE" | description "Diverse"
        IFCSPACE "0-3" | long name "Kjellergang" | object type "IFCSTYLE" | description "Kjellergang"
        IFCSPACE "0-4" | long name "Disponibelt" | object type "IFCSTYLE" | description "Disponibelt"
      IFCBUILDINGSTOREY "Level (1)" | elevation 0.
IFCBEAMTYPE "IFCSTYLE (1)" | BEAM
  IFCBEAMTYPE "Unnamed" | BEAM
IFCBEAMTYPE "IFCSTYLE (2)" | BEAM
  IFCBEAMTYPE "Unnamed" | BEAM
IFCCOLUMNTYPE "IFCSTYLE (3)" | COLUMN
  IFCCOLUMNTYPE "Unnamed" | COLUMN
IFCCOLUMNTYPE "IFCSTYLE (4)" | COLUMN
  IFCCOLUMNTYPE "Unnamed" | COLUMN
IFCCOLUMNTYPE "IFCSTYLE (5)" | COLUMN
  IFCCOLUMNTYPE "Unnamed" | COLUMN
IFCBEAMTYPE "IFCSTYLE (1)" | BEAM
  IFCBEAMTYPE "Unnamed" | BEAM
IFCBEAMTYPE "IFCSTYLE (2)" | BEAM
  IFCBEAMTYPE "Unnamed" | BEAM
IFCBEAMTYPE "IFCSTYLE (3)" | BEAM
  IFCBEAMTYPE "Unnamed" | BEAM
IFCBEAMTYPE "IFCSTYLE (4)" | BEAM
  IFCBEAMTYPE "Unnamed" | BEAM
IFCCOLUMNTYPE "IFCSTYLE (5)" | COLUMN
  IFCCOLUMNTYPE "Unnamed" | COLUMN
IFCCOLUMNTYPE "IFCSTYLE (6)" | COLUMN
  IFCCOLUMNTYPE "Unnamed" | COLUMN
IFCCOLUMNTYPE "IFCSTYLE (7)" | COLUMN
  IFCCOLUMNTYPE "Unnamed" | COLUMN
IFCCOLUMNTYPE "IFCSTYLE (8)" | COLUMN
  IFCCOLUMNTYPE "Unnamed" | COLUMN
IFCCOLUMNTYPE "IFCSTYLE (9)" | COLUMN
  IFCCOLUMNTYPE "Unnamed" | COLUMN

Types
  IFCWALLTYPE "IFCSTYLE (1)" | 8 occurrences | property sets: Pset_ADT_WallStyle
  IFCWINDOWSTYLE "D-51-1000-1400" | 4 occurrences | property sets: Pset_ADT_WindowStyle
  IFCDOORSTYLE "D-16-900-2100" | 6 occurrences | property sets: Pset_ADT_DoorStyle
  IFCWALLTYPE "IFCSTYLE (2)" | 6 occurrences | property sets: Pset_ADT_WallStyle
  IFCWALLTYPE "IFCSTYLE (3)" | 6 occurrences | property sets: Pset_ADT_WallStyle
  IFCWALLTYPE "IFCSTYLE (4)" | 3 occurrences | material: layers "IFCSTYLE (4)" ("68 mm enkelt bindingsverk heltre impregnert" 86.99999749660492) | property sets: Pset_ADT_WallStyle
  IFCSLABTYPE "Floor-100" | FLOOR | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "Floor-100 (2)" | FLOOR | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "Floor-100 (3)" | FLOOR | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "Floor-100 (4)" | FLOOR | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "Floor-100 (5)" | FLOOR | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "Floor-14" | FLOOR | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "Floor-20" | FLOOR | 1 occurrence | material: layers "Floor-20" ("22 mm terrassebord" 21.99999988079071, "148 mm bjelke" 148.0000019073486) | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (0)" | ROOF | 1 occurrence | material: layers "IFCSTYLE (0)" ("12mm taktro" 12.00000010430813, "48mm lekt/luftespalte" 48.00000041723251, "2mm vindsperre" 2.000000094994903, "198mm taksperr og isolasjon" 197.9999989271164) | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (1)" | ROOF | 1 occurrence | material: layers "IFCSTYLE (1)" ("12mm taktro" 12.00000010430813, "48mm lekt/luftespalte" 48.00000041723251, "2mm vindsperre" 2.000000094994903, "198mm taksperr og isolasjon" 197.9999989271164) | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (2)" | ROOF | 1 occurrence | material: layers "IFCSTYLE (2)" ("12mm taktro" 12.00000010430813, "48mm lekt/luftespalte" 48.00000041723251, "2mm vindsperre" 2.000000094994903, "198mm taksperr og isolasjon" 197.9999989271164) | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (3)" | ROOF | 1 occurrence | material: layers "IFCSTYLE (3)" ("12mm taktro" 12.00000010430813, "48mm lekt/luftespalte" 48.00000041723251, "2mm vindsperre" 2.000000094994903, "198mm taksperr og isolasjon" 197.9999989271164) | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (4)" | ROOF | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (5)" | ROOF | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (6)" | ROOF | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (7)" | ROOF | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (8)" | ROOF | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (9)" | ROOF | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (10)" | ROOF | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (11)" | ROOF | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (12)" | ROOF | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (13)" | ROOF | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (14)" | ROOF | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCBEAMTYPE "IFCSTYLE (1)" | BEAM | 1 occurrence | property sets: Pset_ADT_BeamStyle
  IFCBEAMTYPE "IFCSTYLE (2)" | BEAM | 1 occurrence | property sets: Pset_ADT_BeamStyle
  IFCCOLUMNTYPE "IFCSTYLE (3)" | COLUMN | 1 occurrence | property sets: Pset_ADT_ColumnStyle
  IFCCOLUMNTYPE "IFCSTYLE (4)" | COLUMN | 1 occurrence | property sets: Pset_ADT_ColumnStyle
  IFCCOLUMNTYPE "IFCSTYLE (5)" | COLUMN | 1 occurrence | property sets: Pset_ADT_ColumnStyle
  IFCWALLTYPE "IFCSTYLE (1)" | 14 occurrences | material: layers "IFCSTYLE (1)" ("19 mm liggende, utvendig panel m/dobbelfals" 18.99999938905239, "23 mm utlekting på fasade c/c 60" 23.00000004470348, "12 mm asfaltimpregnert trefiberplate" 12.00000010430813, "148 mm enkelt bindingsverk heltre isolert" 148.0000019073486, "13 mm gipsplate innvendig kledning" 13.0000002682209) | property sets: Pset_ADT_WallStyle
  IFCWINDOWSTYLE "D-33-1100-1700" | 6 occurrences | property sets: Pset_ADT_WindowStyle
  IFCDOORSTYLE "D-336-1000-2100" | 6 occurrences | property sets: Pset_ADT_DoorStyle
  IFCWALLTYPE "IFCSTYLE (2)" | 2 occurrences | material: layers "IFCSTYLE (2)" ("13 mm gipsplate innvendig kledning" 13.0000002682209, "98 mm enkelt bindingsverk heltre" 97.99999743700028, "13 mm gipsplate innvendig kledning" 13.0000002682209) | property sets: Pset_ADT_WallStyle
  IFCWALLTYPE "IFCSTYLE (3)" | 5 occurrences | material: layers "IFCSTYLE (3)" ("12 mm spon" 13.0000002682209, "68 mm enkelt bindingsverk heltre" 68.00000369548798, "12 mm spon" 13.0000002682209) | property sets: Pset_ADT_WallStyle
  IFCWALLTYPE "IFCSTYLE (4)" | 1 occurrence | material: layers "IFCSTYLE (4)" ("10 mm puss" 9.999999776482582, "108 mm tegl" 108.0000028014183, "10 mm puss" 9.999999776482582) | property sets: Pset_ADT_WallStyle
  IFCWALLTYPE "IFCSTYLE (5)" | 4 occurrences | material: layers "IFCSTYLE (5)" ("68 mm enkelt bindingsverk heltre impregnert" 86.99999749660492) | property sets: Pset_ADT_WallStyle
  IFCSLABTYPE "Floor-14" | FLOOR | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (0)" | ROOF | 1 occurrence | material: layers "IFCSTYLE (0)" ("12mm taktro" 12.00000010430813, "48mm lekt/luftespalte" 48.00000041723251, "2mm vindsperre" 2.000000094994903, "198mm taksperr og isolasjon" 197.9999989271164) | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (1)" | ROOF | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (2)" | ROOF | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCSLABTYPE "IFCSTYLE (3)" | ROOF | 1 occurrence | property sets: Pset_ADT_SlabStyle
  IFCBEAMTYPE "IFCSTYLE (1)" | BEAM | 1 occurrence | property sets: Pset_ADT_BeamStyle
  IFCBEAMTYPE "IFCSTYLE (2)" | BEAM | 1 occurrence | property sets: Pset_ADT_BeamStyle
  IFCBEAMTYPE "IFCSTYLE (3)" | BEAM | 1 occurrence | property sets: Pset_ADT_BeamStyle
  IFCBEAMTYPE "IFCSTYLE (4)" | BEAM | 1 occurrence | property sets: Pset_ADT_BeamStyle
  IFCCOLUMNTYPE "IFCSTYLE (5)" | COLUMN | 1 occurrence | property sets: Pset_ADT_ColumnStyle
  IFCCOLUMNTYPE "IFCSTYLE (6)" | COLUMN | 1 occurrence | property sets: Pset_ADT_ColumnStyle
  IFCCOLUMNTYPE "IFCSTYLE (7)" | COLUMN | 1 occurrence | property sets: Pset_ADT_ColumnStyle
  IFCCOLUMNTYPE "IFCSTYLE (8)" | COLUMN | 1 occurrence | property sets: Pset_ADT_ColumnStyle
  IFCCOLUMNTYPE "IFCSTYLE (9)" | COLUMN | 1 occurrence | property sets: Pset_ADT_ColumnStyle
  IFCWALLTYPE "IFCSTYLE (1)" | 12 occurrences | property sets: Pset_ADT_WallStyle
  IFCWINDOWSTYLE "D-11-1000-400" | 4 occurrences | property sets: Pset_ADT_WindowStyle
  IFCWALLTYPE "IFCSTYLE (2)" | 15 occurrences | property sets: Pset_ADT_WallStyle
  IFCWALLTYPE "IFCSTYLE (3)" | 2 occurrences | material: layers "IFCSTYLE (3)" ("150 mm betong" 150.0000059604645) | property sets: Pset_ADT_WallStyle
  IFCDOORSTYLE "D-0-900-2100" | 3 occurrences | property sets: Pset_ADT_DoorStyle
  IFCWALLTYPE "IFCSTYLE (4)" | 2 occurrences | material: layers "IFCSTYLE (4)" ("68 mm enkelt bindingsverk heltre isolert" 68.00000369548798, "13 mm gipsplate innvendig kledning" 13.0000002682209) | property sets: Pset_ADT_WallStyle
  IFCWALLTYPE "IFCSTYLE (5)" | 1 occurrence | material: layers "IFCSTYLE (5)" ("12 mm spon" 13.0000002682209, "68 mm enkelt bindingsverk heltre isolert" 68.00000369548798, "12 mm spon" 13.0000002682209) | property sets: Pset_ADT_WallStyle
  IFCSLABTYPE "Floor-31" | FLOOR | 1 occurrence | material: layers "Floor-31" ("50 mm betong" 50.00000074505806, "50 mm isolasjon" 50.00000074505806, "150 mm isolasjon" 150.0000059604645) | property sets: Pset_ADT_SlabStyle

Property sets
  PSET_ACA_DISPLAY_SET | properties | on 1 object (1 IFCPROJECT)
    ACA_DISPLAY_CONFIG_ON_EXPORT = "Medium Detail" (IFCLABEL)
    ACA_DISPLAY_SET_ON_EXPORT = "Model" (IFCLABEL)
  Pset_WallCommon | properties | on 22 objects (11 IFCWALL, 11 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "WT-227" (IFCLABEL)
  Pset_WallCommon | properties | on 15 objects (15 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "WT-163" (IFCLABEL)
  Pset_WallCommon | properties | on 12 objects (12 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "WT-250" (IFCLABEL)
  Pset_WallCommon | properties | on 11 objects (6 IFCWALL, 5 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "WT-45" (IFCLABEL)
  Pset_WallCommon | properties | on 8 objects (6 IFCWALL, 2 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "WT-3" (IFCLABEL)
  Pset_WallCommon | properties | on 7 objects (7 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "WT-1230" (IFCLABEL)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "WT-101" (IFCLABEL)
  Pset_WallCommon | properties | on 2 objects (1 IFCWALL, 1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "WT-169" (IFCLABEL)
  Pset_WallCommon: 2 more contents on 2 objects not shown
  Pset_ADT_Wall | properties | on 22 objects (11 IFCWALL, 11 IFCWALLSTANDARDCASE)
    BaseThickness = 215.0000017136335 (IFCREAL)
    CleanUpRadius = 0. (IFCREAL)
  Pset_ADT_Wall | properties | on 15 objects (15 IFCWALL)
    BaseThickness = 110.9999977052212 (IFCREAL)
    CleanUpRadius = 0. (IFCREAL)
  Pset_ADT_Wall | properties | on 12 objects (6 IFCWALL, 6 IFCWALLSTANDARDCASE)
    BaseThickness = 94.00000423192978 (IFCREAL)
    CleanUpRadius = 0. (IFCREAL)
  Pset_ADT_Wall | properties | on 12 objects (12 IFCWALL)
    BaseThickness = 200.0000029802322 (IFCREAL)
    CleanUpRadius = 0. (IFCREAL)
  Pset_ADT_Wall | properties | on 8 objects (6 IFCWALL, 2 IFCWALLSTANDARDCASE)
    BaseThickness = 123.9999979734421 (IFCREAL)
    CleanUpRadius = 0. (IFCREAL)
  Pset_ADT_Wall | properties | on 7 objects (7 IFCWALLSTANDARDCASE)
    BaseThickness = 86.99999749660492 (IFCREAL)
    CleanUpRadius = 0. (IFCREAL)
  Pset_ADT_Wall | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    BaseThickness = 150.0000059604645 (IFCREAL)
    CleanUpRadius = 0. (IFCREAL)
  Pset_ADT_Wall | properties | on 2 objects (1 IFCWALL, 1 IFCWALLSTANDARDCASE)
    BaseThickness = 81.00000396370888 (IFCREAL)
    CleanUpRadius = 0. (IFCREAL)
  Pset_ADT_Wall: 1 more content on 1 objects not shown
  Wall quantities | quantities | on 2 objects (2 IFCWALLSTANDARDCASE)
    GrossSideAreaRight = 1.628400087356567 [MILLI SQUARE_METRE]
  Wall quantities | quantities | on 1 object (1 IFCWALL)
    GrossSideAreaRight = 4.391821384429932 [MILLI SQUARE_METRE]
  Wall quantities | quantities | on 1 object (1 IFCWALL)
    GrossSideAreaRight = 1.350827693939209 [MILLI SQUARE_METRE]
  Wall quantities | quantities | on 1 object (1 IFCWALL)
    GrossSideAreaRight = 8.583591461181641 [MILLI SQUARE_METRE]
  Wall quantities | quantities | on 1 object (1 IFCWALL)
    GrossSideAreaRight = 1.350828886032105 [MILLI SQUARE_METRE]
  Wall quantities | quantities | on 1 object (1 IFCWALL)
    GrossSideAreaRight = 4.3918137550354 [MILLI SQUARE_METRE]
  Wall quantities | quantities | on 1 object (1 IFCWALL)
    GrossSideAreaRight = 20.16152000427246 [MILLI SQUARE_METRE]
  Wall quantities | quantities | on 1 object (1 IFCWALL)
    GrossSideAreaRight = 12.55915927886963 [MILLI SQUARE_METRE]
  Wall quantities: 72 more contents on 72 objects not shown
  Pset_WindowCommon | properties | on 5 objects (5 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "WI-51-1000-1399" (IFCLABEL)
  Pset_WindowCommon | properties | on 4 objects (4 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "WI-11-1000-400" (IFCLABEL)
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "WI-51-1000-1200" (IFCLABEL)
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "WI-33-1100-1700" (IFCLABEL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "WI-34-1700-1700" (IFCLABEL)
  Pset_DoorCommon | properties | on 11 objects (11 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "DO-0-899-2099" (IFCLABEL)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "DO-16-899-2099" (IFCLABEL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "DO-30-550-800" (IFCLABEL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "DO-336-1000-2099" (IFCLABEL)
  Pset_ADT_Door | properties | on 15 objects (15 IFCDOOR)
    OpenPercent = 50. (IFCREAL)
  Pset_SlabCommon | properties | on 19 objects (19 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Roof-1-40.00" (IFCLABEL)
  Pset_SlabCommon | properties | on 9 objects (9 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Floor-1" (IFCLABEL)
  Pset_ADT_Slab | properties | on 6 objects (6 IFCSLAB)
    BaseThickness = 141.9999970821664 (IFCREAL)
  Pset_ADT_Slab | properties | on 5 objects (5 IFCSLAB)
    BaseThickness = 109.9999975413084 (IFCREAL)
  Pset_ADT_Slab | properties | on 5 objects (5 IFCSLAB)
    BaseThickness = 259.9999995436519 (IFCREAL)
  Pset_ADT_Slab | properties | on 5 objects (5 IFCSLAB)
    BaseThickness = 119.9999991804361 (IFCREAL)
  Pset_ADT_Slab | properties | on 3 objects (3 IFCSLAB)
    BaseThickness = 141.0000026226044 (IFCREAL)
  Pset_ADT_Slab | properties | on 2 objects (2 IFCSLAB)
    BaseThickness = 314.0000104904175 (IFCREAL)
  Pset_ADT_Slab | properties | on 1 object (1 IFCSLAB)
    BaseThickness = 170.0000017881393 (IFCREAL)
  Pset_ADT_Slab | properties | on 1 object (1 IFCSLAB)
    BaseThickness = 250. (IFCREAL)
  Slab quantities | quantities | on 1 object (1 IFCSLAB)
    GrossFootprintArea = 1.817513108253479 [MILLI SQUARE_METRE]
    NetFootprintArea = 0. [MILLI SQUARE_METRE]
  Slab quantities | quantities | on 1 object (1 IFCSLAB)
    GrossFootprintArea = 1.817508578300476 [MILLI SQUARE_METRE]
    NetFootprintArea = 0. [MILLI SQUARE_METRE]
  Slab quantities | quantities | on 1 object (1 IFCSLAB)
    GrossFootprintArea = 5.135023593902588 [MILLI SQUARE_METRE]
    NetFootprintArea = 0. [MILLI SQUARE_METRE]
  Slab quantities | quantities | on 1 object (1 IFCSLAB)
    GrossFootprintArea = 0.7921023964881897 [MILLI SQUARE_METRE]
    NetFootprintArea = 0. [MILLI SQUARE_METRE]
  Slab quantities | quantities | on 1 object (1 IFCSLAB)
    GrossFootprintArea = 0.7921021580696106 [MILLI SQUARE_METRE]
    NetFootprintArea = 0. [MILLI SQUARE_METRE]
  Slab quantities | quantities | on 1 object (1 IFCSLAB)
    GrossFootprintArea = 75.23998260498047 [MILLI SQUARE_METRE]
    NetFootprintArea = 4.024855613708496 [MILLI SQUARE_METRE]
  Slab quantities | quantities | on 1 object (1 IFCSLAB)
    GrossFootprintArea = 5.427395343780518 [MILLI SQUARE_METRE]
    NetFootprintArea = 0. [MILLI SQUARE_METRE]
  Slab quantities | quantities | on 1 object (1 IFCSLAB)
    GrossFootprintArea = 54.59223937988281 [MILLI SQUARE_METRE]
    NetFootprintArea = 0. [MILLI SQUARE_METRE]
  Slab quantities: 20 more contents on 20 objects not shown
  Beam-2 | properties | on 6 objects (6 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Beam-2" (IFCLABEL)
    Slope = 0. (IFCREAL)
    Span = 0. (IFCREAL)
  Column-2 | properties | on 8 objects (8 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Column-2" (IFCLABEL)
    Slope = 0. (IFCREAL)
  Pset_SpaceCommon | properties | on 2 objects (2 IFCSPACE)
    Reference = "Disponibelt" (IFCLABEL)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Soverom 1" (IFCLABEL)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Soverom 2" (IFCLABEL)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Soverom 3" (IFCLABEL)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Bad" (IFCLABEL)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Kott" (IFCLABEL)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Loftstue" (IFCLABEL)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Reference = "Stue/trapp" (IFCLABEL)
  Pset_SpaceCommon: 6 more contents on 6 objects not shown
  SpaceObjects | properties | on 1 object (1 IFCSPACE)
    Description = "Soverom 1" (IFCLABEL)
    Increment = 1 (IFCINTEGER)
    Level (no value)
    Name = "Soverom 1" (IFCLABEL)
    Number = "2-1" (IFCLABEL)
    NumberProjectBased (no value)
    Remarks (no value)
  SpaceObjects | properties | on 1 object (1 IFCSPACE)
    Description = "Soverom 2" (IFCLABEL)
    Increment = 2 (IFCINTEGER)
    Level (no value)
    Name = "Soverom 2" (IFCLABEL)
    Number = "2-2" (IFCLABEL)
    NumberProjectBased (no value)
    Remarks (no value)
  SpaceObjects | properties | on 1 object (1 IFCSPACE)
    Description = "Soverom 3" (IFCLABEL)
    Increment = 3 (IFCINTEGER)
    Level (no value)
    Name = "Soverom 3" (IFCLABEL)
    Number = "2-3" (IFCLABEL)
    NumberProjectBased (no value)
    Remarks (no value)
  SpaceObjects | properties | on 1 object (1 IFCSPACE)
    Description = "Bad" (IFCLABEL)
    Increment = 4 (IFCINTEGER)
    Level (no value)
    Name = "Bad" (IFCLABEL)
    Number = "2-4" (IFCLABEL)
    NumberProjectBased (no value)
    Remarks (no value)
  SpaceObjects | properties | on 1 object (1 IFCSPACE)
    Description = "Kott" (IFCLABEL)
    Increment = 5 (IFCINTEGER)
    Level (no value)
    Name = "Kott" (IFCLABEL)
    Number = "2-5" (IFCLABEL)
    NumberProjectBased (no value)
    Remarks (no value)
  SpaceObjects | properties | on 1 object (1 IFCSPACE)
    Description = "Loftstue" (IFCLABEL)
    Increment = 6 (IFCINTEGER)
    Level (no value)
    Name = "Loftstue" (IFCLABEL)
    Number = "2-6" (IFCLABEL)
    NumberProjectBased (no value)
    Remarks (no value)
  SpaceObjects | properties | on 1 object (1 IFCSPACE)
    Description = "Stue/trapp" (IFCLABEL)
    Increment = 1 (IFCINTEGER)
    Level (no value)
    Name = "Stue/trapp" (IFCLABEL)
    Number = "1-1" (IFCLABEL)
    NumberProjectBased (no value)
    Remarks (no value)
  SpaceObjects | properties | on 1 object (1 IFCSPACE)
    Description = "Kjøkken" (IFCLABEL)
    Increment = 2 (IFCINTEGER)
    Level (no value)
    Name = "Kjøkken" (IFCLABEL)
    Number = "1-2" (IFCLABEL)
    NumberProjectBased (no value)
    Remarks (no value)
  SpaceObjects: 7 more contents on 7 objects not shown
  Pset_ADT_Space | properties | on 14 objects (14 IFCSPACE)
    CeilingHeight = 2400.000095367432 (IFCREAL)
    CeilingThickness = 0. (IFCREAL)
    FloorThickness = 0. (IFCREAL)
    HeightAboveCeiling = 0. (IFCREAL)
    HeightBelowFloor = 0. (IFCREAL)
  Pset_ADT_Space | properties | on 1 object (1 IFCSPACE)
    CeilingHeight = 1372.376332237922 (IFCREAL)
    CeilingThickness = 0. (IFCREAL)
    FloorThickness = 0. (IFCREAL)
    HeightAboveCeiling = 0. (IFCREAL)
    HeightBelowFloor = 0. (IFCREAL)
  Space quantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 15.02932167053223 [MILLI SQUARE_METRE]
  Space quantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 10.78326988220215 [MILLI SQUARE_METRE]
  Space quantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 11.83974170684815 [MILLI SQUARE_METRE]
  Space quantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 9.53177547454834 [MILLI SQUARE_METRE]
  Space quantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 1.978416323661804 [MILLI SQUARE_METRE]
  Space quantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 17.45182800292969 [MILLI SQUARE_METRE]
  Space quantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 35.7994270324707 [MILLI SQUARE_METRE]
  Space quantities | quantities | on 1 object (1 IFCSPACE)
    GrossFloorArea = 18.38284873962402 [MILLI SQUARE_METRE]
  Space quantities: 7 more contents on 7 objects not shown
  Pset_ADT_WallStyle | properties | on 14 type objects
    IsBoundaryForAutomaticSpaces = TRUE (IFCBOOLEAN)
  Pset_ADT_WindowStyle | properties | on 3 type objects
    AdjustToWallWidth = FALSE (IFCBOOLEAN)
    GlassThickness = 10. (IFCREAL)
    IsBoundaryForAutomaticSpaces = FALSE (IFCBOOLEAN)
    SashDepth = 0. (IFCREAL)
    SashWidth = 0. (IFCREAL)
  Pset_ADT_DoorStyle | properties | on 3 type objects
    AdjustToWallWidth = FALSE (IFCBOOLEAN)
    DoorThickness = 50. (IFCREAL)
    GlassThickness = 10. (IFCREAL)
    IsBoundaryForAutomaticSpaces = FALSE (IFCBOOLEAN)
    StopDepth = 0. (IFCREAL)
    StopWidth = 0. (IFCREAL)
  Pset_ADT_SlabStyle | properties | on 28 type objects
    IsBoundaryForAutomaticSpaces = FALSE (IFCBOOLEAN)
  Pset_ADT_BeamStyle | properties | on 6 type objects
    IsBoundaryForAutomaticSpaces = FALSE (IFCBOOLEAN)
  Pset_ADT_ColumnStyle | properties | on 8 type objects
    IsBoundaryForAutomaticSpaces = FALSE (IFCBOOLEAN)