IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, QuantityTakeOffAddOnView]"
File name: "Project Number"
Time stamp: "2016-02-24T15:52:24"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20140903_1530(x64) - Exporter 15.5.0.0 - Alternate UI 15.5.0.0"
Application: "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)"

People and organizations
  Person "mxfm2" of Organization (no name given)
  Owner history of Person "mxfm2" of Organization (no name given) | application "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)" | change NOCHANGE | created 1456329097 (2016-02-24T15:51:37Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Westminster", "London", "UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 5 elements
          3 x IFCWALL | type IFCWALLTYPE "Basic Wall:Wall-Ext_102Bwk-75Ins-100LBlk-12P" | object type "Basic Wall:Wall-Ext_102Bwk-75Ins-100LBlk-12P:216762" | names: "Basic Wall:Wall-Ext_102Bwk-75Ins-100LBlk-12P:289323", "Basic Wall:Wall-Ext_102Bwk-75Ins-100LBlk-12P:289522", "Basic Wall:Wall-Ext_102Bwk-75Ins-100LBlk-12P:289615" | material: materials ("Brick, Common", "Fiberglass Batt", "Concrete Masonry Units _Low Density", "Plaster") | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "2270x2050mm" | object type "2270x2050mm" | names: "Doors_Garage_Horz_Pnl:2270x2050mm:292003" | material: materials ("Door - Handle", "Door - Panel", "Door - Frame/Mullion") | property sets: Pset_DoorCommon, BaseQuantities, Constraints, Dimensions, Identity Data, Other
          1 x IFCSLAB | object type "Floor:Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" | FLOOR | names: "Floor:Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC:292083" | material: layers "Floor:Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" ("Concrete, Sand/Cement Screed" 65., "Rigid insulation" 80., "Air" 150., "Concrete Masonry, Floor Block" 100., "Concrete, Precast" 75.) | property sets: Pset_SlabCommon, BaseQuantities, Constraints, Dimensions, Other, Phasing
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 4000.
        contains 1 element
          1 x IFCROOF | object type "Basic Roof:Roof_Pitched-50SS-220Ins-20MPan-225Purl:217696" | names: "Basic Roof:Roof_Pitched-50SS-220Ins-20MPan-225Purl:289870" | material: "Roofing, Standing Seam" | property sets: Pset_RoofCommon, Constraints, Construction, Dimensions, Other, Phasing

Types
  IFCWALLTYPE "Basic Wall:Wall-Ext_102Bwk-75Ins-100LBlk-12P" | 3 occurrences | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "2270x2050mm" | ROLLINGUP | 1 occurrence | material: materials ("Door - Handle", "Door - Panel", "Door - Frame/Mullion") | property sets: Doors_Garage_Horz_Pnl:2270x2050mm:292003, Analytical Properties, Construction, Dimensions, Graphics, Identity Data

Property sets
  Constraints | properties | on 3 objects (3 IFCWALL)
    Base Constraint = "Level: Level 0" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = TRUE (IFCBOOLEAN)
    Unconnected Height = 8000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCROOF)
    Extrusion End = -7290.00000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    Extrusion Start = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Level Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Reference Level = "Level: Level 1" (IFCLABEL)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Work Plane = "Basic Wall : Wall-Ext_102Bwk-75Ins-100LBlk-12P" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCDOOR)
    Level = "Level: Level 0" (IFCLABEL)
    Sill Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCSLAB)
    Height Offset From Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Level = "Level: Level 0" (IFCLABEL)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 4000. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCWALL)
    Area = 16.3033998007736 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 7000. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 4.71080199496184 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALL)
    Area = 9.66769309441192 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3989.99999999998 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 2.80308669415347 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCWALL)
    Area = 12.8121535529665 (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 7144.99999999999 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 3.70025560200886 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCROOF)
    Area = 57.6639453165302 (IFCAREAMEASURE) [SQUARE_METRE]
    Thickness = 115. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 6.59328586324319 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCDOOR)
    Area = 5.49275549999993 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.222342870499999 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCSLAB)
    Area = 45.14 (IFCAREAMEASURE) [SQUARE_METRE]
    Perimeter = 27000. (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 470. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 21.2158 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 type object
    Cavity Closer Depth = 75. (IFCLENGTHMEASURE) [MILLI METRE]
    Cavity Closer Offset from Ext = 102.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Cavity Closer Width = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Door Panel Thickness = 44. (IFCLENGTHMEASURE) [MILLI METRE]
    FrameOffset - External = 25. (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Z Distance = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2050. (IFCLENGTHMEASURE) [MILLI METRE]
    Rough Height = 2050. (IFCLENGTHMEASURE) [MILLI METRE]
    Rough Width = 2270. (IFCLENGTHMEASURE) [MILLI METRE]
    Structural Tolerance = 6.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Thickness = 44. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance = 3. (IFCLENGTHMEASURE) [MILLI METRE]
    Undercut = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 2270. (IFCLENGTHMEASURE) [MILLI METRE]
  Other | properties | on 3 objects (3 IFCWALL)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: Wall-Ext_102Bwk-75Ins-100LBlk-12P" (IFCLABEL)
    Family and Type = "Basic Wall: Wall-Ext_102Bwk-75Ins-100LBlk-12P" (IFCLABEL)
    Type = "Basic Wall: Wall-Ext_102Bwk-75Ins-100LBlk-12P" (IFCLABEL)
    Type Id = "Basic Wall: Wall-Ext_102Bwk-75Ins-100LBlk-12P" (IFCLABEL)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Circle Head - Project Datum" (IFCLABEL)
    Family and Type = "Level: Circle Head - Project Datum" (IFCLABEL)
    Type = "Level: Circle Head - Project Datum" (IFCLABEL)
    Type Id = "Level: Circle Head - Project Datum" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCROOF)
    Category = "Roofs" (IFCLABEL)
    Family = "Basic Roof: Roof_Pitched-50SS-220Ins-20MPan-225Purl" (IFCLABEL)
    Family and Type = "Basic Roof: Roof_Pitched-50SS-220Ins-20MPan-225Purl" (IFCLABEL)
    Type = "Basic Roof: Roof_Pitched-50SS-220Ins-20MPan-225Purl" (IFCLABEL)
    Type Id = "Basic Roof: Roof_Pitched-50SS-220Ins-20MPan-225Purl" (IFCLABEL)
  Other | properties | on 1 object (1 IFCDOOR)
    Category = "Doors" (IFCLABEL)
    Family = "Doors_Garage_Horz_Pnl: 2270x2050mm" (IFCLABEL)
    Family and Type = "Doors_Garage_Horz_Pnl: 2270x2050mm" (IFCLABEL)
    Head Height = 2050. (IFCLENGTHMEASURE) [MILLI METRE]
    Host Id = "Basic Wall: Wall-Ext_102Bwk-75Ins-100LBlk-12P" (IFCLABEL)
    Type = "Doors_Garage_Horz_Pnl: 2270x2050mm" (IFCLABEL)
    Type Id = "Doors_Garage_Horz_Pnl: 2270x2050mm" (IFCLABEL)
  Other | properties | on 1 object (1 IFCSLAB)
    Category = "Floors" (IFCLABEL)
    Family = "Floor: Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" (IFCLABEL)
    Family and Type = "Floor: Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" (IFCLABEL)
    Type = "Floor: Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" (IFCLABEL)
    Type Id = "Floor: Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" (IFCLABEL)
  Other | properties | on 1 object (1 IFCROOF)
    Category = "Roofs" (IFCLABEL)
    Family Name = "Basic Roof" (IFCTEXT)
  Other: 3 more contents on 1 objects not shown
  Phasing | properties | on 6 objects (3 IFCWALL, 1 IFCDOOR, 1 IFCROOF, 1 IFCSLAB)
    Phase Created = "New Construction" (IFCLABEL)
  Structural | properties | on 3 objects (3 IFCWALL)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Structural | properties | on 1 object (1 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Wall-Ext_102Bwk-75Ins-100LBlk-12P" (IFCIDENTIFIER)
    ThermalTransmittance = 0.235926059936681 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 56.4255809937324 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Roof_Pitched-50SS-220Ins-20MPan-225Purl" (IFCIDENTIFIER)
    TotalArea = 57.6639453165302 (IFCAREAMEASURE) [SQUARE_METRE]
  Construction | properties | on 1 object (1 IFCROOF)
    Fascia Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rafter Cut = "Plumb Cut" (IFCIDENTIFIER)
  Construction | properties | on 1 object (1 IFCROOF)
    Default Thickness = 115. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 object (1 IFCSLAB)
    Default Thickness = 470. (IFCLENGTHMEASURE) [MILLI METRE]
    Function = "Interior" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 290. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Both" (IFCIDENTIFIER)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Wall Closure = "By host" (IFCIDENTIFIER)
    Wrap Layers (Ext) from Ext = 102.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Wrap Layers (Int) from Ext = 177.5 (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "2270x2050mm" (IFCIDENTIFIER)
    ThermalTransmittance = 3.7021 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  BaseQuantities | quantities | on 1 object (1 IFCDOOR)
    Area = 5.49275549999993 [SQUARE_METRE]
    Height = 2050. [MILLI METRE]
    Width = 2270. [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCSLAB)
    GrossArea = 45.14 [SQUARE_METRE]
    GrossVolume = 21215.8 [CUBIC_METRE]
    Perimeter = 27000. [MILLI METRE]
    Width = 470. [MILLI METRE]
  BaseQuantities | quantities | on 1 object (1 IFCOPENINGELEMENT)
    Depth = 290. [MILLI METRE]
    Height = 2270. [MILLI METRE]
    Width = 2050. [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Type Name = "Circle Head - Project Datum" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCDOOR)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 0" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCROOF)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Roof_Pitched-50SS-220Ins-20MPan-225Purl" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCSLAB)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Keynote = "E60/130" (IFCTEXT)
    Type Name = "Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Keynote = "F10" (IFCTEXT)
    Type Name = "Wall-Ext_102Bwk-75Ins-100LBlk-12P" (IFCTEXT)
  Identity Data: 1 more content on 0 objects not shown
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" (IFCIDENTIFIER)
    ThermalTransmittance = 0.117437608263296 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 2 (IFCINTEGER)
  Analytical Properties | properties | on 1 object (1 IFCROOF)
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 1.74387350932981 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 0.573436086189709 (IFCREAL)
    Thermal mass = 295971.2 (IFCREAL)
  Analytical Properties | properties | on 1 object (1 IFCSLAB)
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.117437608263296 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 8.51515979240645 (IFCREAL)
    Thermal mass = 365549.43 (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 0.235926059936681 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 4.23861611671209 (IFCREAL)
    Thermal mass = 300303. (IFCREAL)
  Analytical Properties | properties | on 1 type object
    Analytic Construction = "Metal" (IFCTEXT)
    Heat Transfer Coefficient (U) = 3.7021 (IFCREAL)
    Solar Heat Gain Coefficient = 0. (IFCREAL)
    Thermal Resistance (R) = 0.270116960643959 (IFCREAL)
    Visual Light Transmittance = 0. (IFCREAL)
  Graphics | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "Anno_Level_Head_Circle: Standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = FALSE (IFCBOOLEAN)
  Graphics | properties | on 1 object (1 IFCROOF)
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Graphics | properties | on 1 object (1 IFCSLAB)
    Coarse Scale Fill Color = 0 (IFCINTEGER)
    Coarse Scale Fill Pattern = "Solid fill" (IFCLABEL)
  Graphics | properties | on 1 type object
    Coarse Scale Fill Color = 12632256 (IFCINTEGER)
    Coarse Scale Fill Pattern = "Solid fill" (IFCLABEL)
  Graphics | properties | on 1 type object
    Vis - Cavity Closers = TRUE (IFCBOOLEAN)
    Vis - Ironmongery = TRUE (IFCBOOLEAN)
  Materials and Finishes | properties | on 1 object (1 IFCSLAB)
    Structural Material = "Concrete Masonry, Floor Block" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Structural Material = "Concrete Masonry Units _Low Density" (IFCLABEL)
  Materials and Finishes | properties | on 1 type object
    Material Door = "Door - Panel" (IFCLABEL)
    Material Frame = "Door - Frame/Mullion" (IFCLABEL)
    Material Ironmongery = "Door - Handle" (IFCLABEL)
  Doors_Garage_Horz_Pnl:2270x2050mm:292003 | predefined | on 2 type objects