IFC building model
Schema: "IFC2X3"
Description: "IFC2X3"
File name: "ullandhaug_tower.Ifc"
Time stamp: "2008-12-09T20:03:35"
Author: "ST"
Organization: "Data Design System ASA"
Preprocessor: "DDS-IFC v2.0"
Originating system: "DDS-CAD Version 6.5 Release build 18/11-2008"
Authorization: "DDS"
Application: "DDS-CAD Building" version "DDS-CAD Building" identifier "DDS-CAD" by Organization "DDS"
Application: "DDS-CAD Electrical - Building" version "Version 6.5 Release build 18/11-2008" identifier "DDS-CAD Electrical - Building Version 6.5 Release build 18/11-2008" by Organization "DDS"
Application: "DDS-CAD Electrical - Ventilasjon" version "Version 6.5 Release build 18/11-2008" identifier "DDS-CAD Electrical - Ventilasjon Version 6.5 Release build 18/11-2008" by Organization "DDS"
Application: "DDS-CAD Electrical - R>r" version "Version 6.5 Release build 18/11-2008" identifier "DDS-CAD Electrical - R>r Version 6.5 Release build 18/11-2008" by Organization "DDS"

People and organizations
  Person "Stian" "Tonheim" of Organization "DDS"
  3 x Person "ST" "_ST" of Organization "DDS"
  Owner history of Person "Stian" "Tonheim" of Organization "DDS" | application "DDS-CAD Building" version "DDS-CAD Building" identifier "DDS-CAD" by Organization "DDS" | change NOCHANGE | created 1228848953 (2008-12-09T18:55:53Z)
  Owner history of Person "ST" "_ST" of Organization "DDS" | application "DDS-CAD Electrical - Building" version "Version 6.5 Release build 18/11-2008" identifier "DDS-CAD Electrical - Building Version 6.5 Release build 18/11-2008" by Organization "DDS" | change NOCHANGE | created 1228848953 (2008-12-09T18:55:53Z)
  Owner history of Person "ST" "_ST" of Organization "DDS" | application "DDS-CAD Electrical - Ventilasjon" version "Version 6.5 Release build 18/11-2008" identifier "DDS-CAD Electrical - Ventilasjon Version 6.5 Release build 18/11-2008" by Organization "DDS" | change NOCHANGE | created 1228848982 (2008-12-09T18:56:22Z)
  Owner history of Person "ST" "_ST" of Organization "DDS" | application "DDS-CAD Electrical - R>r" version "Version 6.5 Release build 18/11-2008" identifier "DDS-CAD Electrical - R>r Version 6.5 Release build 18/11-2008" by Organization "DDS" | change NOCHANGE | created 1228848988 (2008-12-09T18:56:28Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  ELECTRICRESISTANCEUNIT: OHM
  POWERUNIT: WATT
  MASSUNIT: GRAM
  SOLIDANGLEUNIT: STERADIAN
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  PRESSUREUNIT: PASCAL
  LUMINOUSFLUXUNIT: LUMEN
  ILLUMINANCEUNIT: LUX
  FREQUENCYUNIT: HERTZ
  VOLUMEUNIT: CUBIC_METRE
  TIMEUNIT: SECOND
  VOLUMETRICFLOWRATEUNIT: derived
  THERMALTRANSMITTANCEUNIT: derived
  PLANEANGLEUNIT: DEGREE (conversion based)

Spatial structure
IFCPROJECT "Tower" | description "Ullandhaug Tower"
  IFCSITE "Ullandhaug" | latitude 60° 23′ 0″ | longitude 5° 20′ 0″ | elevation above sea level 0. | postal address OFFICE: "Bergen"
    IFCBUILDING "Tower"
      IFCBUILDINGSTOREY "Sea level" | elevation 0. | description "Sea level"
      IFCBUILDINGSTOREY "Level 1" | elevation 72. | description "1.etasje"
        contains 158 elements
          3 x IFCSLAB | FLOOR | names: "Golv mot grunn n'ringsbygg" | descriptions: "Golv mot grunn n'ringsbygg" | material: layers "ML-Golv mot grunn n'ringsbygg - 0.250" ("Layer-Golv mot grunn n'ringsbygg" 0.25) | property sets: Slab quantities, Pset_SlabCommon
          22 x IFCWALLSTANDARDCASE | names: "Yttervegg 20.0cm", "Innervegg 10.0cm" | descriptions: "Yttervegg 20.0cm", "Innervegg 10.0cm" | material: layers "ML-Yttervegg 20.0cm - 0.200" ("Layer-Yttervegg 20.0cm" 0.2000000029802322); layers "ML-Innervegg 10.0cm - 0.100" ("Layer-Innervegg 10.0cm" 0.1) | property sets: Wall quantities, Pset_WallCommon
          1 x IFCDOOR | type IFCDOORSTYLE "Innerd>r 2 fl>yet - 1.400x2.100" | object type "Innerd>r 2 fl>yet" | names: "Innerd>r 2 fl>yet - 1.400x2.100" | descriptions: "Innerd>r 2 fl>yet - 1.400x2.100" | property sets: Pset_DoorCommon
          1 x IFCDOOR | type IFCDOORSTYLE "Innerd>r 2 fl>yet - 1.400x2.100" | object type "Innerd>r 2 fl>yet" | names: "Innerd>r 2 fl>yet - 1.400x2.100" | descriptions: "Innerd>r 2 fl>yet - 1.400x2.100" | property sets: Pset_DoorCommon
          15 x IFCBUILDINGELEMENTPROXY | names: "BinObjCom"
          1 x IFCBUILDINGELEMENTPROXY | object type "AF020301_646_AF-070307-100_1019" | names: "Komponenter" | descriptions: "Trapp rett"
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | property sets: Pset_DDS
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          1 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | property sets: Pset_DDS
          28 x IFCDISTRIBUTIONPORT
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          4 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | property sets: Pset_DDS
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          8 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | property sets: Pset_DDS
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          2 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          56 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
        IFCSPACE "001" | long name "Oppholdsrom" | INTERNAL | description "Oppholdsrom"
        IFCSPACE "002" | long name "Oppholdsrom" | INTERNAL | description "Oppholdsrom"
      IFCBUILDINGSTOREY "Level 2" | elevation 79. | description "2.etasje"
        contains 121 elements
          4 x IFCSLAB | FLOOR | names: "Hulldekke 320 mm" | descriptions: "Hulldekke 320 mm" | material: layers "ML-Hulldekke 320 mm - 0.320" ("Layer-Hulldekke 320 mm" 0.3199999928474426) | property sets: Slab quantities, Pset_SlabCommon
          14 x IFCWALLSTANDARDCASE | names: "Yttervegg 20.0cm", "Innervegg 10.0cm" | descriptions: "Yttervegg 20.0cm", "Innervegg 10.0cm" | material: layers "ML-Yttervegg 20.0cm - 0.200" ("Layer-Yttervegg 20.0cm" 0.2000000029802322); layers "ML-Innervegg 10.0cm - 0.100" ("Layer-Innervegg 10.0cm" 0.1) | property sets: Pset_WallCommon, Wall quantities
          5 x IFCBUILDINGELEMENTPROXY | names: "BinObjCom"
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          6 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | property sets: Pset_DDS
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          16 x IFCDISTRIBUTIONPORT
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          2 x IFCFLOWFITTING | type IFCDUCTFITTINGTYPE "BE2000" | property sets: Pset_DDS
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          1 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
          65 x IFCFLOWSEGMENT | type IFCDUCTSEGMENTTYPE "SS1002" | property sets: Pset_FlowSegmentDuctSegment, Pset_DDS
        IFCSPACE "001" | long name "Oppholdsrom" | INTERNAL | description "Oppholdsrom"
        IFCSPACE "002" | long name "Oppholdsrom" | INTERNAL | description "Oppholdsrom"
      IFCBUILDINGSTOREY "Level 3" | elevation 85. | description "3.etasje"
        contains 48 elements
          4 x IFCSLAB | FLOOR | names: "Hulldekke 320 mm" | descriptions: "Hulldekke 320 mm" | material: layers "ML-Hulldekke 320 mm - 0.320" ("Layer-Hulldekke 320 mm" 0.3199999928474426) | property sets: Pset_SlabCommon, Slab quantities
          28 x IFCWALLSTANDARDCASE | names: "Yttervegg 20.0cm", "B>lgeblekk", "Innervegg 10.0cm" (+2 more) | descriptions: "Yttervegg 20.0cm", "B>lgeblekk", "Innervegg 10.0cm" (+2 more) | material: layers "ML-Yttervegg 20.0cm - 0.200" ("Layer-Yttervegg 20.0cm" 0.2000000029802322); layers "ML-B>lgeblekk - 0.200" ("Layer-B>lgeblekk" 0.2); layers "ML-Innervegg 10.0cm - 0.100" ("Layer-Innervegg 10.0cm" 0.1); layers "ML-Yttervegg 15.0cm - 0.150" ("Layer-Yttervegg 15.0cm" 0.1500005722045898); layers "ML-Yttervegg 15.0cm - 0.149" ("Layer-Yttervegg 15.0cm" 0.1490441709756851); layers "ML-Yttervegg 20.0cm - 0.199" ("Layer-Yttervegg 20.0cm" 0.1992644965648651) | property sets: Pset_WallCommon, Wall quantities
          16 x IFCWINDOW | object type "Isolerglass" | names: "Isolerglass - 1.400x1.400" | descriptions: "Isolerglass - 1.400x1.400" | property sets: Pset_WindowCommon
        IFCSPACE "001" | long name "Tower room" | INTERNAL | description "Tower room"
        IFCSPACE "002" | long name "Space1" | INTERNAL | description "Space1"
        IFCSPACE "003" | long name "Space2" | INTERNAL | description "Space2"
      IFCBUILDINGSTOREY "Level 4" | elevation 91.
        contains 48 elements
          4 x IFCSLAB | FLOOR | names: "Hulldekke 320 mm" | descriptions: "Hulldekke 320 mm" | material: layers "ML-Hulldekke 320 mm - 0.320" ("Layer-Hulldekke 320 mm" 0.3199999928474426) | property sets: Pset_SlabCommon, Slab quantities
          28 x IFCWALLSTANDARDCASE | names: "Yttervegg 20.0cm", "B>lgeblekk", "Innervegg 10.0cm" (+2 more) | descriptions: "Yttervegg 20.0cm", "B>lgeblekk", "Innervegg 10.0cm" (+2 more) | material: layers "ML-Yttervegg 20.0cm - 0.200" ("Layer-Yttervegg 20.0cm" 0.2000000029802322); layers "ML-B>lgeblekk - 0.200" ("Layer-B>lgeblekk" 0.2); layers "ML-Innervegg 10.0cm - 0.100" ("Layer-Innervegg 10.0cm" 0.1); layers "ML-Yttervegg 15.0cm - 0.150" ("Layer-Yttervegg 15.0cm" 0.1500005722045898); layers "ML-Yttervegg 15.0cm - 0.149" ("Layer-Yttervegg 15.0cm" 0.1490441709756851); layers "ML-Yttervegg 20.0cm - 0.199" ("Layer-Yttervegg 20.0cm" 0.1992644965648651) | property sets: Pset_WallCommon, Wall quantities
          16 x IFCWINDOW | object type "Isolerglass" | names: "Isolerglass - 1.400x1.400" | descriptions: "Isolerglass - 1.400x1.400" | property sets: Pset_WindowCommon
        IFCSPACE "001" | long name "Tower room" | INTERNAL | description "Tower room"
        IFCSPACE "002" | long name "Space1" | INTERNAL | description "Space1"
        IFCSPACE "003" | long name "Space2" | INTERNAL | description "Space2"
      IFCBUILDINGSTOREY "Level 5" | elevation 97.
        contains 48 elements
          4 x IFCSLAB | FLOOR | names: "Hulldekke 320 mm" | descriptions: "Hulldekke 320 mm" | material: layers "ML-Hulldekke 320 mm - 0.320" ("Layer-Hulldekke 320 mm" 0.3199999928474426) | property sets: Pset_SlabCommon, Slab quantities
          28 x IFCWALLSTANDARDCASE | names: "Yttervegg 20.0cm", "B>lgeblekk", "Innervegg 10.0cm" (+2 more) | descriptions: "Yttervegg 20.0cm", "B>lgeblekk", "Innervegg 10.0cm" (+2 more) | material: layers "ML-Yttervegg 20.0cm - 0.200" ("Layer-Yttervegg 20.0cm" 0.2000000029802322); layers "ML-B>lgeblekk - 0.200" ("Layer-B>lgeblekk" 0.2); layers "ML-Innervegg 10.0cm - 0.100" ("Layer-Innervegg 10.0cm" 0.1); layers "ML-Yttervegg 15.0cm - 0.150" ("Layer-Yttervegg 15.0cm" 0.1500005722045898); layers "ML-Yttervegg 15.0cm - 0.149" ("Layer-Yttervegg 15.0cm" 0.1490441709756851); layers "ML-Yttervegg 20.0cm - 0.199" ("Layer-Yttervegg 20.0cm" 0.1992644965648651) | property sets: Pset_WallCommon, Wall quantities
          16 x IFCWINDOW | object type "Isolerglass" | names: "Isolerglass - 1.400x1.400" | descriptions: "Isolerglass - 1.400x1.400" | property sets: Pset_WindowCommon
        IFCSPACE "001" | long name "Tower room" | INTERNAL | description "Tower room"
        IFCSPACE "002" | long name "Space1" | INTERNAL | description "Space1"
        IFCSPACE "003" | long name "Space2" | INTERNAL | description "Space2"
      IFCBUILDINGSTOREY "Level 6" | elevation 103.
        contains 50 elements
          4 x IFCSLAB | FLOOR | names: "Hulldekke 320 mm" | descriptions: "Hulldekke 320 mm" | material: layers "ML-Hulldekke 320 mm - 0.320" ("Layer-Hulldekke 320 mm" 0.3199999928474426) | property sets: Pset_SlabCommon, Slab quantities
          28 x IFCWALLSTANDARDCASE | names: "Yttervegg 20.0cm", "B>lgeblekk", "Innervegg 10.0cm" (+2 more) | descriptions: "Yttervegg 20.0cm", "B>lgeblekk", "Innervegg 10.0cm" (+2 more) | material: layers "ML-Yttervegg 20.0cm - 0.200" ("Layer-Yttervegg 20.0cm" 0.2000000029802322); layers "ML-B>lgeblekk - 0.200" ("Layer-B>lgeblekk" 0.2); layers "ML-Innervegg 10.0cm - 0.100" ("Layer-Innervegg 10.0cm" 0.1); layers "ML-Yttervegg 15.0cm - 0.150" ("Layer-Yttervegg 15.0cm" 0.1500005722045898); layers "ML-Yttervegg 15.0cm - 0.149" ("Layer-Yttervegg 15.0cm" 0.1490441709756851); layers "ML-Yttervegg 20.0cm - 0.199" ("Layer-Yttervegg 20.0cm" 0.1992644965648651) | property sets: Pset_WallCommon, Wall quantities
          16 x IFCWINDOW | object type "Isolerglass" | names: "Isolerglass - 1.400x1.400" | descriptions: "Isolerglass - 1.400x1.400" | property sets: Pset_WindowCommon
          2 x IFCBUILDINGELEMENTPROXY | names: "BinObjCom"
        IFCSPACE "001" | long name "Tower room" | INTERNAL | description "Tower room"
        IFCSPACE "002" | long name "Space1" | INTERNAL | description "Space1"
        IFCSPACE "003" | long name "Space2" | INTERNAL | description "Space2"
      IFCBUILDINGSTOREY "Level 7" | elevation 108.9999999928475 | description "tower007"
        contains 80 elements
          4 x IFCSLAB | FLOOR | names: "Hulldekke 320 mm" | descriptions: "Hulldekke 320 mm" | material: layers "ML-Hulldekke 320 mm - 0.320" ("Layer-Hulldekke 320 mm" 0.3199999928474426) | property sets: Pset_SlabCommon, Slab quantities
          20 x IFCWALLSTANDARDCASE | names: "Yttervegg 20.0cm", "Innervegg 10.0cm" | descriptions: "Yttervegg 20.0cm", "Innervegg 10.0cm" | material: layers "ML-Yttervegg 20.0cm - 0.200" ("Layer-Yttervegg 20.0cm" 0.2000000029802322); layers "ML-Innervegg 10.0cm - 0.100" ("Layer-Innervegg 10.0cm" 0.1) | property sets: Pset_WallCommon, Wall quantities
          2 x IFCBUILDINGELEMENTPROXY | names: "BinObjCom"
          23 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS1000" | material: layers "ML-1-ª" stÅlr>r m/gj. sorte DN 32" ("ML-1-ª" stÅlr>r m/gj. sorte DN 32" 0.002) | property sets: Pset_FlowSegmentPipeSegment, Pset_DDS
          5 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS1000" | material: layers "ML-1" stÅlr>r m/gj. sorte DN 25" ("ML-1" stÅlr>r m/gj. sorte DN 25" 0.002) | property sets: Pset_FlowSegmentPipeSegment, Pset_DDS
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_DDS
          16 x IFCDISTRIBUTIONPORT
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_DDS
          2 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "antenne.bin" | property sets: Pset_DDS
        IFCSPACE "001" | long name "Space" | INTERNAL | description "Space"
        IFCSPACE "002" | long name "Space" | INTERNAL | description "Space"
      IFCBUILDINGSTOREY "Level 8" | elevation 114.3200001645088
        contains 79 elements
          4 x IFCSLAB | FLOOR | names: "Hulldekke 320 mm" | descriptions: "Hulldekke 320 mm" | material: layers "ML-Hulldekke 320 mm - 0.320" ("Layer-Hulldekke 320 mm" 0.3199999928474426) | property sets: Pset_SlabCommon, Slab quantities
          20 x IFCWALLSTANDARDCASE | names: "Yttervegg 20.0cm", "Innervegg 10.0cm" | descriptions: "Yttervegg 20.0cm", "Innervegg 10.0cm" | material: layers "ML-Yttervegg 20.0cm - 0.200" ("Layer-Yttervegg 20.0cm" 0.2000000029802322); layers "ML-Innervegg 10.0cm - 0.100" ("Layer-Innervegg 10.0cm" 0.1) | property sets: Pset_WallCommon, Wall quantities
          2 x IFCBUILDINGELEMENTPROXY | names: "BinObjCom"
          23 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS1000" | material: layers "ML-1-ª" stÅlr>r m/gj. sorte DN 32" ("ML-1-ª" stÅlr>r m/gj. sorte DN 32" 0.002) | property sets: Pset_FlowSegmentPipeSegment, Pset_DDS
          5 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS1000" | material: layers "ML-1" stÅlr>r m/gj. sorte DN 25" ("ML-1" stÅlr>r m/gj. sorte DN 25" 0.002) | property sets: Pset_FlowSegmentPipeSegment, Pset_DDS
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_DDS
          16 x IFCDISTRIBUTIONPORT
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_DDS
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "antenne.bin" | property sets: Pset_DDS
        IFCSPACE "001" | long name "Space" | INTERNAL | description "Space"
        IFCSPACE "002" | long name "Space" | INTERNAL | description "Space"
      IFCBUILDINGSTOREY "Level 9" | elevation 119.6400001645088
        contains 82 elements
          4 x IFCSLAB | FLOOR | names: "Hulldekke 320 mm" | descriptions: "Hulldekke 320 mm" | material: layers "ML-Hulldekke 320 mm - 0.320" ("Layer-Hulldekke 320 mm" 0.3199999928474426) | property sets: Pset_SlabCommon, Slab quantities
          20 x IFCWALLSTANDARDCASE | names: "Yttervegg 20.0cm", "Innervegg 10.0cm" | descriptions: "Yttervegg 20.0cm", "Innervegg 10.0cm" | material: layers "ML-Yttervegg 20.0cm - 0.200" ("Layer-Yttervegg 20.0cm" 0.2000000029802322); layers "ML-Innervegg 10.0cm - 0.100" ("Layer-Innervegg 10.0cm" 0.1) | property sets: Pset_WallCommon, Wall quantities
          2 x IFCBUILDINGELEMENTPROXY | names: "BinObjCom"
          23 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS1000" | material: layers "ML-1-ª" stÅlr>r m/gj. sorte DN 32" ("ML-1-ª" stÅlr>r m/gj. sorte DN 32" 0.002) | property sets: Pset_FlowSegmentPipeSegment, Pset_DDS
          5 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS1000" | material: layers "ML-1" stÅlr>r m/gj. sorte DN 25" ("ML-1" stÅlr>r m/gj. sorte DN 25" 0.002) | property sets: Pset_FlowSegmentPipeSegment, Pset_DDS
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_DDS
          16 x IFCDISTRIBUTIONPORT
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_DDS
          4 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "antenne.bin" | property sets: Pset_DDS
        IFCSPACE "001" | long name "Space" | INTERNAL | description "Space"
        IFCSPACE "002" | long name "Space" | INTERNAL | description "Space"
      IFCBUILDINGSTOREY "Level 10" | elevation 124.9600001645088
        contains 80 elements
          4 x IFCSLAB | FLOOR | names: "Hulldekke 320 mm" | descriptions: "Hulldekke 320 mm" | material: layers "ML-Hulldekke 320 mm - 0.320" ("Layer-Hulldekke 320 mm" 0.3199999928474426) | property sets: Pset_SlabCommon, Slab quantities
          20 x IFCWALLSTANDARDCASE | names: "Yttervegg 20.0cm", "Innervegg 10.0cm" | descriptions: "Yttervegg 20.0cm", "Innervegg 10.0cm" | material: layers "ML-Yttervegg 20.0cm - 0.200" ("Layer-Yttervegg 20.0cm" 0.2000000029802322); layers "ML-Innervegg 10.0cm - 0.100" ("Layer-Innervegg 10.0cm" 0.1) | property sets: Pset_WallCommon, Wall quantities
          2 x IFCBUILDINGELEMENTPROXY | names: "BinObjCom"
          23 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS1000" | material: layers "ML-1-ª" stÅlr>r m/gj. sorte DN 32" ("ML-1-ª" stÅlr>r m/gj. sorte DN 32" 0.002) | property sets: Pset_FlowSegmentPipeSegment, Pset_DDS
          5 x IFCFLOWSEGMENT | type IFCPIPESEGMENTTYPE "SS1000" | material: layers "ML-1" stÅlr>r m/gj. sorte DN 25" ("ML-1" stÅlr>r m/gj. sorte DN 25" 0.002) | property sets: Pset_FlowSegmentPipeSegment, Pset_DDS
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_DDS
          16 x IFCDISTRIBUTIONPORT
          4 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "BE2000" | property sets: Pset_DDS
          2 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "antenne.bin" | property sets: Pset_DDS
        IFCSPACE "001" | long name "Space" | INTERNAL | description "Space"
        IFCSPACE "002" | long name "Space" | INTERNAL | description "Space"
      IFCBUILDINGSTOREY "Top level" | elevation 130.2800001573563 | description "tower011"
        contains 16 elements
          2 x IFCSLAB | FLOOR | names: "Hulldekke 320 mm" | descriptions: "Hulldekke 320 mm" | material: layers "ML-Hulldekke 320 mm - 0.320" ("Layer-Hulldekke 320 mm" 0.3199999928474426) | property sets: Pset_SlabCommon, Slab quantities
          10 x IFCWALLSTANDARDCASE | names: "Yttervegg 20.0cm", "Innervegg 10.0cm" | descriptions: "Yttervegg 20.0cm", "Innervegg 10.0cm" | material: layers "ML-Yttervegg 20.0cm - 0.200" ("Layer-Yttervegg 20.0cm" 0.2000000029802322); layers "ML-Innervegg 10.0cm - 0.100" ("Layer-Innervegg 10.0cm" 0.1) | property sets: Pset_WallCommon, Wall quantities
          1 x IFCSLAB | ROOF | names: "Hulldekke" | descriptions: "Hulldekke" | material: layers "ML-Hulldekke - 0.000" ("Layer-Hulldekke" 0.) | property sets: Slab quantities, Pset_SlabCommon
          3 x IFCBUILDINGELEMENTPROXY | names: "BinObjCom"
        IFCSPACE "001" | long name "Oppholdsrom" | INTERNAL | description "Oppholdsrom"

Types
  IFCDOORSTYLE "Innerd>r 2 fl>yet - 1.400x2.100" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDOORSTYLE "Innerd>r 2 fl>yet - 1.400x2.100" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SS-091208194230_1006_15_600_0.42" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rekkverk"
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER010201_000_BEREK5FR_1004_15_600_270_23_0" | BEND | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctFittingTypeCommon | description "Rekt bend frirund / rund"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SS-091208194230_1006_15_600_7.40" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rekkverk"
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER010201_000_BEREK5FR_1004_15_600_90_23_0" | BEND | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctFittingTypeCommon | description "Rekt bend frirund / rund"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SS-091208194230_1006_15_600_28.57" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rekkverk"
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER010201_000_BEREK590_1005_15_600_180_90_0" | BEND | 4 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_DuctFittingTypeCommon | description "Rekt bend 90 rund / rund"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SS-091208194230_1006_15_600_15.69" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rekkverk"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SS-091208194230_1006_15_600_29.66" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rekkverk"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SS-091208194230_1006_15_600_3.64" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rekkverk"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SS-091208194230_1006_15_600_3.91" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rekkverk"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SSREKT_1002_15_100_28.58" | RIGIDSEGMENT | 2 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rektangul'r kanal"
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER010201_000_BEREK590_1005_15_100_180_90_0" | BEND | 14 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_DuctFittingTypeCommon | description "Rekt bend 90 rund / rund"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SSREKT_1002_15_100_15.69" | RIGIDSEGMENT | 2 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rektangul'r kanal"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SSREKT_1002_15_100_29.66" | RIGIDSEGMENT | 2 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rektangul'r kanal"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SSREKT_1002_15_100_3.64" | RIGIDSEGMENT | 2 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rektangul'r kanal"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SSREKT_1002_15_100_3.90" | RIGIDSEGMENT | 2 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rektangul'r kanal"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SSREKT_1002_15_20_1.25" | RIGIDSEGMENT | 56 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rektangul'r kanal"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SSREKT_1002_15_100_2.12" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rektangul'r kanal"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SSREKT_1002_15_100_26.31" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rektangul'r kanal"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SSREKT_1002_15_100_12.77" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rektangul'r kanal"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SSREKT_1002_15_100_26.30" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rektangul'r kanal"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SSREKT_1002_15_100_2.24" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rektangul'r kanal"
  IFCDUCTFITTINGTYPE "BE2000" | element type "BER010201_000_BEREK590_1005_15_100_0_90_0" | BEND | 2 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_DuctFittingTypeCommon | description "Rekt bend 90 rund / rund"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SSREKT_1002_15_100_1.38" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rektangul'r kanal"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SSREKT_1002_15_100_7.96" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rektangul'r kanal"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SSREKT_1002_15_100_1.37" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rektangul'r kanal"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SSREKT_1002_15_100_0.03" | RIGIDSEGMENT | 1 occurrence | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rektangul'r kanal"
  IFCDUCTSEGMENTTYPE "SS1002" | element type "SS020101_002_SSREKT_1002_15_20_0.25" | RIGIDSEGMENT | 65 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_DuctSegmentTypeCommon | description "Rektangul'r kanal"
  IFCPIPESEGMENTTYPE "SS1000" | element type "SS040101_000_1001014_1004" | RIGIDSEGMENT | 92 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_PipeSegmentTypeCommon | description "1-ª" stÅlr>r m/gj. sorte DN 32"
  IFCPIPESEGMENTTYPE "SS1000" | element type "SS040101_000_1001012_1007" | RIGIDSEGMENT | 20 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_PipeSegmentTypeCommon | description "1" stÅlr>r m/gj. sorte DN 25"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010401_000_1010132_1008_90_25" | BEND | 16 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_PipeFittingTypeCommon | description "1" sort stÅl bend 90 DN 25"
  IFCPIPEFITTINGTYPE "BE2000" | element type "BE010401_000_1010134_1005_90_32" | BEND | 16 occurrences | property sets: Pset_ManufacturerTypeInformation, Pset_PipeFittingTypeCommon | description "1-ª" sort stÅl bend 90 DN 32"
  IFCBOILERTYPE "antenne.bin" | element type "GF010101_000_GF-091208190822_1009" | WATER | 9 occurrences | property sets: Pset_ManufacturerTypeInformation | description "Antenna"

Property sets
  Space quantities | quantities | on 4 objects (4 IFCSPACE)
    Area = 26.72000694274902 [SQUARE_METRE]
    AverageClearHeight = 5. [METRE]
    AverageGrossHeight = 5.319999992847443 [METRE]
    AverageHeight = 5.319999992847443 [METRE]
    Volume = 133.6000366210938 [CUBIC_METRE]
  Space quantities | quantities | on 4 objects (4 IFCSPACE)
    Area = 5.078799247741699 [SQUARE_METRE]
    AverageClearHeight = 5. [METRE]
    AverageGrossHeight = 5.320000171661377 [METRE]
    AverageHeight = 5.320000171661377 [METRE]
    Volume = 25.39399719238281 [CUBIC_METRE]
  Space quantities | quantities | on 3 objects (3 IFCSPACE)
    Area = 58.874755859375 [SQUARE_METRE]
    AverageClearHeight = 5.669999828562141 [METRE]
    AverageGrossHeight = 5.999999992847442 [METRE]
    AverageHeight = 5.999999992847442 [METRE]
    Volume = 334.4085998535156 [CUBIC_METRE]
  Space quantities | quantities | on 3 objects (3 IFCSPACE)
    Area = 27.5710391998291 [SQUARE_METRE]
    AverageClearHeight = 5.669999828562141 [METRE]
    AverageGrossHeight = 5.999999992847442 [METRE]
    AverageHeight = 5.999999992847442 [METRE]
    Volume = 156.6035003662109 [CUBIC_METRE]
  Space quantities | quantities | on 3 objects (3 IFCSPACE)
    Area = 5.841201305389404 [SQUARE_METRE]
    AverageClearHeight = 5.659999828785658 [METRE]
    AverageGrossHeight = 5.999999992847442 [METRE]
    AverageHeight = 5.999999992847442 [METRE]
    Volume = 33.17802429199219 [CUBIC_METRE]
  Space quantities | quantities | on 1 object (1 IFCSPACE)
    Area = 176.5799713134766 [SQUARE_METRE]
    AverageClearHeight = 6.629999827593565 [METRE]
    AverageGrossHeight = 6.930000007152557 [METRE]
    AverageHeight = 6.930000007152557 [METRE]
    Volume = 1179.55419921875 [CUBIC_METRE]
  Space quantities | quantities | on 1 object (1 IFCSPACE)
    Area = 242.7899932861328 [SQUARE_METRE]
    AverageClearHeight = 2.949999999254942 [METRE]
    AverageGrossHeight = 3.250000000745058 [METRE]
    AverageHeight = 3.250000000745058 [METRE]
    Volume = 728.3699951171875 [CUBIC_METRE]
  Space quantities | quantities | on 1 object (1 IFCSPACE)
    Area = 26.72000694274902 [SQUARE_METRE]
    AverageClearHeight = 5.679999828338623 [METRE]
    AverageGrossHeight = 6. [METRE]
    AverageHeight = 6. [METRE]
    Volume = 151.7696380615234 [CUBIC_METRE]
  Space quantities: 5 more contents on 5 objects not shown
  Slab quantities | quantities | on 7 objects (7 IFCSLAB)
    SurfaceArea = 26.72000694274902 [SQUARE_METRE]
  Slab quantities | quantities | on 5 objects (5 IFCSLAB)
    SurfaceArea = 31.08000564575195 [SQUARE_METRE]
  Slab quantities | quantities | on 4 objects (4 IFCSLAB)
    SurfaceArea = 102.9723663330078 [SQUARE_METRE]
  Slab quantities | quantities | on 4 objects (4 IFCSLAB)
    SurfaceArea = 58.874755859375 [SQUARE_METRE]
  Slab quantities | quantities | on 4 objects (4 IFCSLAB)
    SurfaceArea = 27.5710391998291 [SQUARE_METRE]
  Slab quantities | quantities | on 4 objects (4 IFCSLAB)
    SurfaceArea = 5.841201305389404 [SQUARE_METRE]
  Slab quantities | quantities | on 4 objects (4 IFCSLAB)
    SurfaceArea = 7.639069080352783 [SQUARE_METRE]
  Slab quantities | quantities | on 4 objects (4 IFCSLAB)
    SurfaceArea = 5.078799247741699 [SQUARE_METRE]
  Slab quantities: 6 more contents on 6 objects not shown
  Pset_SlabCommon | properties | on 39 objects (39 IFCSLAB)
    ThermalTransmittance = 3. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    ThermalTransmittance = 0.3100000023841858 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Wall quantities | quantities | on 10 objects (10 IFCWALLSTANDARDCASE)
    NominalLength = 0.09999991208314897 [METRE]
  Wall quantities | quantities | on 10 objects (10 IFCWALLSTANDARDCASE)
    NominalLength = 1.199999809265139 [METRE]
  Wall quantities | quantities | on 10 objects (10 IFCWALLSTANDARDCASE)
    NominalLength = 0.1000000685453415 [METRE]
  Wall quantities | quantities | on 10 objects (10 IFCWALLSTANDARDCASE)
    NominalLength = 2.00000047683716 [METRE]
  Wall quantities | quantities | on 10 objects (10 IFCWALLSTANDARDCASE)
    NominalLength = 1.5 [METRE]
  Wall quantities | quantities | on 8 objects (8 IFCWALLSTANDARDCASE)
    NominalLength = 0.10000005394377 [METRE]
  Wall quantities | quantities | on 8 objects (8 IFCWALLSTANDARDCASE)
    NominalLength = 0.1004810333251953 [METRE]
  Wall quantities | quantities | on 7 objects (7 IFCWALLSTANDARDCASE)
    NominalLength = 5.200000405311585 [METRE]
  Wall quantities: 54 more contents on 165 objects not shown
  Pset_WallCommon | properties | on 148 objects (148 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Yttervegg 20.0cm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.2000000029802322 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 66 objects (66 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Innervegg 10.0cm" (IFCIDENTIFIER)
    ThermalTransmittance = 2. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 16 objects (16 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "B>lgeblekk" (IFCIDENTIFIER)
    ThermalTransmittance = 0.2000000029802322 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 8 objects (8 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Yttervegg 15.0cm" (IFCIDENTIFIER)
    ThermalTransmittance = 0.2000000029802322 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 2. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_DDS | properties | on 1 object (1 IFCFLOWFITTING)
    Above Sea Level ref. Bottom = "NNUK=74.98 m" (IFCTEXT)
    Above Sea Level ref. Center = "NN=75.58 m" (IFCTEXT)
    Abs. rrykk = "0.0 Pa" (IFCTEXT)
    Building Part = "Building: 0" (IFCTEXT)
    Del nummer = ".020" (IFCTEXT)
    Del streng nummer = ".0000" (IFCTEXT)
    Dimension DN = "15x600" (IFCTEXT)
    Group = "" (IFCTEXT)
    H>yde = "600" (IFCTEXT)
    Hastighet = "0.000000 m/s" (IFCTEXT)
    Hoved streng nummer = "00" (IFCTEXT)
    Iso tykkelse = "iso= 0.000000 mm" (IFCTEXT)
    Isolasjon U-verdi = "0" (IFCTEXT)
    Isolasjon WSVO = "0" (IFCTEXT)
    Layer number = 1200 (IFCINTEGER)
    Lengde = "200.0 m" (IFCTEXT)
    Length = "200" (IFCTEXT)
    Medium = "Beam" (IFCTEXT)
    Mengde (l/s) = "0.00 l/s" (IFCTEXT)
    Mengde (l/t) = "0.000000 l/h" (IFCTEXT)
    Mengde (m/h) = "0.000000 m/h" (IFCTEXT)
    Model Number = "Dra.no: 1" (IFCTEXT)
    Mounting Height = "3.58 m" (IFCTEXT)
    Mtg. Above Slab ref Bottom = "UK= 3.28m RFB" (IFCTEXT)
    Mtg. Above Slab ref Center = "CC= 3.58m RFB" (IFCTEXT)
    Mtg. Below Ceiling ref Center = "CC= 3.10m UKD" (IFCTEXT)
    Mtg. Below Ceiling ref Top = "OK= 2.80m UKD" (IFCTEXT)
    Mtg. above Finished Floor ref Center = "CC= 3.53m FFB" (IFCTEXT)
    Product = "Rekt bend 90 rund / rund" (IFCTEXT)
    Product Number = "BEREK590" (IFCTEXT)
    Project name = "tower" (IFCTEXT)
    R>rdiameter: = "x0.0" (IFCTEXT)
    Room Name = "Bygning" (IFCTEXT)
    Room Number = "001" (IFCTEXT)
    Storey Number = "Storey: 2" (IFCTEXT)
    Vridning = "180.000000" (IFCTEXT)
    Width = "15" (IFCTEXT)
    X = "X=-25.96" (IFCTEXT)
    Y = "Y=11.95" (IFCTEXT)
    Ytter diameter = "15.000000" (IFCTEXT)
  Pset_DDS | properties | on 1 object (1 IFCFLOWFITTING)
    Above Sea Level ref. Bottom = "NNUK=74.98 m" (IFCTEXT)
    Above Sea Level ref. Center = "NN=75.58 m" (IFCTEXT)
    Abs. rrykk = "0.0 Pa" (IFCTEXT)
    Building Part = "Building: 0" (IFCTEXT)
    Del nummer = ".028" (IFCTEXT)
    Del streng nummer = ".0000" (IFCTEXT)
    Dimension DN = "15x600" (IFCTEXT)
    Group = "" (IFCTEXT)
    H>yde = "600" (IFCTEXT)
    Hastighet = "0.000000 m/s" (IFCTEXT)
    Hoved streng nummer = "00" (IFCTEXT)
    Iso tykkelse = "iso= 0.000000 mm" (IFCTEXT)
    Isolasjon U-verdi = "0" (IFCTEXT)
    Isolasjon WSVO = "0" (IFCTEXT)
    Layer number = 1200 (IFCINTEGER)
    Lengde = "200.0 m" (IFCTEXT)
    Length = "200" (IFCTEXT)
    Medium = "Beam" (IFCTEXT)
    Mengde (l/s) = "0.00 l/s" (IFCTEXT)
    Mengde (l/t) = "0.000000 l/h" (IFCTEXT)
    Mengde (m/h) = "0.000000 m/h" (IFCTEXT)
    Model Number = "Dra.no: 1" (IFCTEXT)
    Mounting Height = "3.58 m" (IFCTEXT)
    Mtg. Above Slab ref Bottom = "UK= 3.28m RFB" (IFCTEXT)
    Mtg. Above Slab ref Center = "CC= 3.58m RFB" (IFCTEXT)
    Mtg. Below Ceiling ref Center = "CC= 3.10m UKD" (IFCTEXT)
    Mtg. Below Ceiling ref Top = "OK= 2.80m UKD" (IFCTEXT)
    Mtg. above Finished Floor ref Center = "CC= 3.53m FFB" (IFCTEXT)
    Product = "Rekt bend 90 rund / rund" (IFCTEXT)
    Product Number = "BEREK590" (IFCTEXT)
    Project name = "tower" (IFCTEXT)
    R>rdiameter: = "x0.0" (IFCTEXT)
    Room Name = "Bygning" (IFCTEXT)
    Room Number = "001" (IFCTEXT)
    Storey Number = "Storey: 2" (IFCTEXT)
    Vridning = "180.000000" (IFCTEXT)
    Width = "15" (IFCTEXT)
    X = "X=-25.96" (IFCTEXT)
    Y = "Y=-3.96" (IFCTEXT)
    Ytter diameter = "15.000000" (IFCTEXT)
  Pset_DDS | properties | on 1 object (1 IFCFLOWFITTING)
    Above Sea Level ref. Bottom = "NNUK=74.98 m" (IFCTEXT)
    Above Sea Level ref. Center = "NN=75.58 m" (IFCTEXT)
    Abs. rrykk = "0.0 Pa" (IFCTEXT)
    Building Part = "Building: 0" (IFCTEXT)
    Del nummer = ".043" (IFCTEXT)
    Del streng nummer = ".0000" (IFCTEXT)
    Dimension DN = "15x600" (IFCTEXT)
    Group = "" (IFCTEXT)
    H>yde = "600" (IFCTEXT)
    Hastighet = "0.000000 m/s" (IFCTEXT)
    Hoved streng nummer = "00" (IFCTEXT)
    Iso tykkelse = "iso= 0.000000 mm" (IFCTEXT)
    Isolasjon U-verdi = "0" (IFCTEXT)
    Isolasjon WSVO = "0" (IFCTEXT)
    Layer number = 1200 (IFCINTEGER)
    Lengde = "200.0 m" (IFCTEXT)
    Length = "200" (IFCTEXT)
    Medium = "Beam" (IFCTEXT)
    Mengde (l/s) = "0.00 l/s" (IFCTEXT)
    Mengde (l/t) = "0.000000 l/h" (IFCTEXT)
    Mengde (m/h) = "0.000000 m/h" (IFCTEXT)
    Model Number = "Dra.no: 1" (IFCTEXT)
    Mounting Height = "3.58 m" (IFCTEXT)
    Mtg. Above Slab ref Bottom = "UK= 3.28m RFB" (IFCTEXT)
    Mtg. Above Slab ref Center = "CC= 3.58m RFB" (IFCTEXT)
    Mtg. Below Ceiling ref Center = "CC= 3.10m UKD" (IFCTEXT)
    Mtg. Below Ceiling ref Top = "OK= 2.80m UKD" (IFCTEXT)
    Mtg. above Finished Floor ref Center = "CC= 3.53m FFB" (IFCTEXT)
    Product = "Rekt bend 90 rund / rund" (IFCTEXT)
    Product Number = "BEREK590" (IFCTEXT)
    Project name = "tower" (IFCTEXT)
    R>rdiameter: = "x0.0" (IFCTEXT)
    Room Name = "Bygning" (IFCTEXT)
    Room Number = "001" (IFCTEXT)
    Storey Number = "Storey: 2" (IFCTEXT)
    Vridning = "180.000000" (IFCTEXT)
    Width = "15" (IFCTEXT)
    X = "X=3.91" (IFCTEXT)
    Y = "Y=-3.96" (IFCTEXT)
    Ytter diameter = "15.000000" (IFCTEXT)
  Pset_DDS | properties | on 1 object (1 IFCFLOWFITTING)
    Above Sea Level ref. Bottom = "NNUK=74.98 m" (IFCTEXT)
    Above Sea Level ref. Center = "NN=75.58 m" (IFCTEXT)
    Abs. rrykk = "0.0 Pa" (IFCTEXT)
    Building Part = "Building: 0" (IFCTEXT)
    Del nummer = ".045" (IFCTEXT)
    Del streng nummer = ".0000" (IFCTEXT)
    Dimension DN = "15x600" (IFCTEXT)
    Group = "" (IFCTEXT)
    H>yde = "600" (IFCTEXT)
    Hastighet = "0.000000 m/s" (IFCTEXT)
    Hoved streng nummer = "00" (IFCTEXT)
    Iso tykkelse = "iso= 0.000000 mm" (IFCTEXT)
    Isolasjon U-verdi = "0" (IFCTEXT)
    Isolasjon WSVO = "0" (IFCTEXT)
    Layer number = 1200 (IFCINTEGER)
    Lengde = "200.0 m" (IFCTEXT)
    Length = "200" (IFCTEXT)
    Medium = "Beam" (IFCTEXT)
    Mengde (l/s) = "0.00 l/s" (IFCTEXT)
    Mengde (l/t) = "0.000000 l/h" (IFCTEXT)
    Mengde (m/h) = "0.000000 m/h" (IFCTEXT)
    Model Number = "Dra.no: 1" (IFCTEXT)
    Mounting Height = "3.58 m" (IFCTEXT)
    Mtg. Above Slab ref Bottom = "UK= 3.28m RFB" (IFCTEXT)
    Mtg. Above Slab ref Center = "CC= 3.58m RFB" (IFCTEXT)
    Mtg. Below Ceiling ref Center = "CC= 3.10m UKD" (IFCTEXT)
    Mtg. Below Ceiling ref Top = "OK= 2.80m UKD" (IFCTEXT)
    Mtg. above Finished Floor ref Center = "CC= 3.53m FFB" (IFCTEXT)
    Product = "Rekt bend 90 rund / rund" (IFCTEXT)
    Product Number = "BEREK590" (IFCTEXT)
    Project name = "tower" (IFCTEXT)
    R>rdiameter: = "x0.0" (IFCTEXT)
    Room Name = "Bygning" (IFCTEXT)
    Room Number = "001" (IFCTEXT)
    Storey Number = "Storey: 2" (IFCTEXT)
    Vridning = "180.000000" (IFCTEXT)
    Width = "15" (IFCTEXT)
    X = "X=3.91" (IFCTEXT)
    Y = "Y=-0.10" (IFCTEXT)
    Ytter diameter = "15.000000" (IFCTEXT)
  Pset_DDS | properties | on 1 object (1 IFCFLOWSEGMENT)
    Above Sea Level ref. Bottom = "NNUK=76.10 m" (IFCTEXT)
    Above Sea Level ref. Center = "NN=76.15 m" (IFCTEXT)
    Abs. trykk = "0.0 Pa" (IFCTEXT)
    Building Part = "Building: 0" (IFCTEXT)
    Del nummer = ".001" (IFCTEXT)
    Delstreng nummer = ".0000" (IFCTEXT)
    Dimension DN = "15x100" (IFCTEXT)
    Flowsegment thickness: = "x0.0" (IFCTEXT)
    Group = "" (IFCTEXT)
    Hastighet = "0.00 m/s" (IFCTEXT)
    Height = "100" (IFCTEXT)
    Hoved streng nummer = "00" (IFCTEXT)
    Iso tykkelse = "iso= 0.000000 mm" (IFCTEXT)
    Isolasjon U-verdi = "0" (IFCTEXT)
    Isolasjon WSVO = "0" (IFCTEXT)
    Layer number = 1200 (IFCINTEGER)
    Length = "29" (IFCTEXT)
    Manufacturer = "DDS" (IFCTEXT)
    Medium = "Beam" (IFCTEXT)
    Mengde = "0.0 m/h" (IFCTEXT)
    Model Number = "Dra.no: 1" (IFCTEXT)
    Mounting Height = "4.15 m" (IFCTEXT)
    Mtg. Above Slab ref Bottom = "UK= 4.10m RFB" (IFCTEXT)
    Mtg. Above Slab ref Center = "CC= 4.15m RFB" (IFCTEXT)
    Mtg. Below Ceiling ref Center = "CC= 2.53m UKD" (IFCTEXT)
    Mtg. Below Ceiling ref Top = "OK= 2.48m UKD" (IFCTEXT)
    Mtg. above Finished Floor ref Center = "CC= 4.10m FFB" (IFCTEXT)
    Product = "Rektangul'r kanal" (IFCTEXT)
    Product Number = "SSREKT" (IFCTEXT)
    Project name = "tower" (IFCTEXT)
    Room Name = "Bygning" (IFCTEXT)
    Room Number = "001" (IFCTEXT)
    Storey Number = "Storey: 2" (IFCTEXT)
    Width = "15" (IFCTEXT)
    X = "X=2.73" (IFCTEXT)
    Y = "Y=11.95" (IFCTEXT)
  Pset_DDS | properties | on 1 object (1 IFCFLOWFITTING)
    Above Sea Level ref. Bottom = "NNUK=76.05 m" (IFCTEXT)
    Above Sea Level ref. Center = "NN=76.15 m" (IFCTEXT)
    Abs. rrykk = "0.0 Pa" (IFCTEXT)
    Building Part = "Building: 0" (IFCTEXT)
    Del nummer = ".015" (IFCTEXT)
    Del streng nummer = ".0000" (IFCTEXT)
    Dimension DN = "15x100" (IFCTEXT)
    Group = "" (IFCTEXT)
    H>yde = "100" (IFCTEXT)
    Hastighet = "0.000000 m/s" (IFCTEXT)
    Hoved streng nummer = "00" (IFCTEXT)
    Iso tykkelse = "iso= 0.000000 mm" (IFCTEXT)
    Isolasjon U-verdi = "0" (IFCTEXT)
    Isolasjon WSVO = "0" (IFCTEXT)
    Layer number = 1200 (IFCINTEGER)
    Lengde = "200.0 m" (IFCTEXT)
    Length = "200" (IFCTEXT)
    Medium = "Beam" (IFCTEXT)
    Mengde (l/s) = "0.00 l/s" (IFCTEXT)
    Mengde (l/t) = "0.000000 l/h" (IFCTEXT)
    Mengde (m/h) = "0.000000 m/h" (IFCTEXT)
    Model Number = "Dra.no: 1" (IFCTEXT)
    Mounting Height = "4.15 m" (IFCTEXT)
    Mtg. Above Slab ref Bottom = "UK= 4.10m RFB" (IFCTEXT)
    Mtg. Above Slab ref Center = "CC= 4.15m RFB" (IFCTEXT)
    Mtg. Below Ceiling ref Center = "CC= 2.53m UKD" (IFCTEXT)
    Mtg. Below Ceiling ref Top = "OK= 2.48m UKD" (IFCTEXT)
    Mtg. above Finished Floor ref Center = "CC= 4.10m FFB" (IFCTEXT)
    Product = "Rekt bend 90 rund / rund" (IFCTEXT)
    Product Number = "BEREK590" (IFCTEXT)
    Project name = "tower" (IFCTEXT)
    R>rdiameter: = "x0.0" (IFCTEXT)
    Room Name = "Bygning" (IFCTEXT)
    Room Number = "001" (IFCTEXT)
    Storey Number = "Storey: 2" (IFCTEXT)
    Vridning = "180.000000" (IFCTEXT)
    Width = "15" (IFCTEXT)
    X = "X=-25.96" (IFCTEXT)
    Y = "Y=11.95" (IFCTEXT)
    Ytter diameter = "15.000000" (IFCTEXT)
  Pset_DDS | properties | on 1 object (1 IFCFLOWSEGMENT)
    Above Sea Level ref. Bottom = "NNUK=76.10 m" (IFCTEXT)
    Above Sea Level ref. Center = "NN=76.15 m" (IFCTEXT)
    Abs. trykk = "0.0 Pa" (IFCTEXT)
    Building Part = "Building: 0" (IFCTEXT)
    Del nummer = ".016" (IFCTEXT)
    Delstreng nummer = ".0000" (IFCTEXT)
    Dimension DN = "15x100" (IFCTEXT)
    Flowsegment thickness: = "x0.0" (IFCTEXT)
    Group = "" (IFCTEXT)
    Hastighet = "0.00 m/s" (IFCTEXT)
    Height = "100" (IFCTEXT)
    Hoved streng nummer = "00" (IFCTEXT)
    Iso tykkelse = "iso= 0.000000 mm" (IFCTEXT)
    Isolasjon U-verdi = "0" (IFCTEXT)
    Isolasjon WSVO = "0" (IFCTEXT)
    Layer number = 1200 (IFCINTEGER)
    Length = "16" (IFCTEXT)
    Manufacturer = "DDS" (IFCTEXT)
    Medium = "Beam" (IFCTEXT)
    Mengde = "0.0 m/h" (IFCTEXT)
    Model Number = "Dra.no: 1" (IFCTEXT)
    Mounting Height = "4.15 m" (IFCTEXT)
    Mtg. Above Slab ref Bottom = "UK= 4.10m RFB" (IFCTEXT)
    Mtg. Above Slab ref Center = "CC= 4.15m RFB" (IFCTEXT)
    Mtg. Below Ceiling ref Center = "CC= 2.53m UKD" (IFCTEXT)
    Mtg. Below Ceiling ref Top = "OK= 2.48m UKD" (IFCTEXT)
    Mtg. above Finished Floor ref Center = "CC= 4.10m FFB" (IFCTEXT)
    Product = "Rektangul'r kanal" (IFCTEXT)
    Product Number = "SSREKT" (IFCTEXT)
    Project name = "tower" (IFCTEXT)
    Room Name = "Bygning" (IFCTEXT)
    Room Number = "001" (IFCTEXT)
    Storey Number = "Storey: 2" (IFCTEXT)
    Width = "15" (IFCTEXT)
    X = "X=-25.96" (IFCTEXT)
    Y = "Y=11.85" (IFCTEXT)
  Pset_DDS | properties | on 1 object (1 IFCFLOWFITTING)
    Above Sea Level ref. Bottom = "NNUK=76.05 m" (IFCTEXT)
    Above Sea Level ref. Center = "NN=76.15 m" (IFCTEXT)
    Abs. rrykk = "0.0 Pa" (IFCTEXT)
    Building Part = "Building: 0" (IFCTEXT)
    Del nummer = ".023" (IFCTEXT)
    Del streng nummer = ".0000" (IFCTEXT)
    Dimension DN = "15x100" (IFCTEXT)
    Group = "" (IFCTEXT)
    H>yde = "100" (IFCTEXT)
    Hastighet = "0.000000 m/s" (IFCTEXT)
    Hoved streng nummer = "00" (IFCTEXT)
    Iso tykkelse = "iso= 0.000000 mm" (IFCTEXT)
    Isolasjon U-verdi = "0" (IFCTEXT)
    Isolasjon WSVO = "0" (IFCTEXT)
    Layer number = 1200 (IFCINTEGER)
    Lengde = "200.0 m" (IFCTEXT)
    Length = "200" (IFCTEXT)
    Medium = "Beam" (IFCTEXT)
    Mengde (l/s) = "0.00 l/s" (IFCTEXT)
    Mengde (l/t) = "0.000000 l/h" (IFCTEXT)
    Mengde (m/h) = "0.000000 m/h" (IFCTEXT)
    Model Number = "Dra.no: 1" (IFCTEXT)
    Mounting Height = "4.15 m" (IFCTEXT)
    Mtg. Above Slab ref Bottom = "UK= 4.10m RFB" (IFCTEXT)
    Mtg. Above Slab ref Center = "CC= 4.15m RFB" (IFCTEXT)
    Mtg. Below Ceiling ref Center = "CC= 2.53m UKD" (IFCTEXT)
    Mtg. Below Ceiling ref Top = "OK= 2.48m UKD" (IFCTEXT)
    Mtg. above Finished Floor ref Center = "CC= 4.10m FFB" (IFCTEXT)
    Product = "Rekt bend 90 rund / rund" (IFCTEXT)
    Product Number = "BEREK590" (IFCTEXT)
    Project name = "tower" (IFCTEXT)
    R>rdiameter: = "x0.0" (IFCTEXT)
    Room Name = "Bygning" (IFCTEXT)
    Room Number = "001" (IFCTEXT)
    Storey Number = "Storey: 2" (IFCTEXT)
    Vridning = "180.000000" (IFCTEXT)
    Width = "15" (IFCTEXT)
    X = "X=-25.96" (IFCTEXT)
    Y = "Y=-3.96" (IFCTEXT)
    Ytter diameter = "15.000000" (IFCTEXT)
  Pset_DDS: 314 more contents on 314 objects not shown
  Pset_FlowSegmentDuctSegment | properties | on 65 objects (65 IFCFLOWSEGMENT)
    Length = 0.25 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 56 objects (56 IFCFLOWSEGMENT)
    Length = 1.24999988079071 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 3 objects (3 IFCFLOWSEGMENT)
    Length = 15.69351959228516 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 3 objects (3 IFCFLOWSEGMENT)
    Length = 29.65839576721191 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 28.58164787292481 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 3.642147064208984 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 2 objects (2 IFCFLOWSEGMENT)
    Length = 3.904401063919067 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment | properties | on 1 object (1 IFCFLOWSEGMENT)
    Length = 0.4177225828170776 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentDuctSegment: 13 more contents on 13 objects not shown
  Pset_WindowCommon | properties | on 64 objects (64 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 1.299999952316284 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_FlowSegmentPipeSegment | properties | on 72 objects (72 IFCFLOWSEGMENT)
    Length = 1. (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Length = 1.622433304786682 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Length = 13.7859001159668 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Length = 8.338711738586426 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Length = 13.78512954711914 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Length = 1.570222973823547 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Length = 1.61543333530426 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment | properties | on 4 objects (4 IFCFLOWSEGMENT)
    Length = 13.77190113067627 (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_FlowSegmentPipeSegment: 3 more contents on 12 objects not shown
  Storey quantities | quantities | on 3 objects (3 IFCBUILDINGSTOREY)
    TotalHeight = 6.319999992847443 [METRE]
  Storey quantities | quantities | on 2 objects (2 IFCBUILDINGSTOREY)
    TotalHeight = 6.32 [METRE]
  Storey quantities | quantities | on 2 objects (2 IFCBUILDINGSTOREY)
    TotalHeight = 5.640000000000001 [METRE]
  Storey quantities | quantities | on 1 object (1 IFCBUILDINGSTOREY)
    TotalHeight = 72.31999999999999 [METRE]
  Storey quantities | quantities | on 1 object (1 IFCBUILDINGSTOREY)
    TotalHeight = 7.25 [METRE]
  Storey quantities | quantities | on 1 object (1 IFCBUILDINGSTOREY)
    TotalHeight = 5.64000016450882 [METRE]
  Storey quantities | quantities | on 1 object (1 IFCBUILDINGSTOREY)
    TotalHeight = 5.639999992847443 [METRE]
  Storey quantities | quantities | on 1 object (1 IFCBUILDINGSTOREY)
    TotalHeight = 3.319999985694885 [METRE]
  Pset_ManufacturerTypeInformation | properties | on 16 type objects
    ArticleNumber = "SSREKT" (IFCIDENTIFIER)
    Manufacturer = "DDS" (IFCLABEL)
    ModelReference = "Rektangul'r kanal" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 7 type objects
    ArticleNumber = "SS-091208194230" (IFCIDENTIFIER)
    Manufacturer = "DDS" (IFCLABEL)
    ModelReference = "Rekkverk" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 3 type objects
    ArticleNumber = "BEREK590" (IFCIDENTIFIER)
    ModelReference = "Rekt bend 90 rund / rund" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 2 type objects
    ArticleNumber = "BEREK5FR" (IFCIDENTIFIER)
    ModelReference = "Rekt bend frirund / rund" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    ArticleNumber = "1001014" (IFCIDENTIFIER)
    ModelReference = "1-ª" stÅlr>r m/gj. sorte DN 32" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    ArticleNumber = "1001012" (IFCIDENTIFIER)
    ModelReference = "1" stÅlr>r m/gj. sorte DN 25" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    ArticleNumber = "1010132" (IFCIDENTIFIER)
    ModelReference = "1" sort stÅl bend 90 DN 25" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 type object
    ArticleNumber = "1010134" (IFCIDENTIFIER)
    ModelReference = "1-ª" sort stÅl bend 90 DN 32" (IFCLABEL)
  Pset_ManufacturerTypeInformation: 1 more content on 0 objects not shown
  Pset_DuctSegmentTypeCommon | properties | on 14 type objects
    NominalDiameterOrWidth = [0.015] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = [0.1] (IFCPOSITIVELENGTHMEASURE) [METRE]
    Shape in {"RECTANGULAR"} (IFCTEXT)
  Pset_DuctSegmentTypeCommon | properties | on 7 type objects
    NominalDiameterOrWidth = [0.015] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = [0.6] (IFCPOSITIVELENGTHMEASURE) [METRE]
    Shape in {"RECTANGULAR"} (IFCTEXT)
  Pset_DuctSegmentTypeCommon | properties | on 2 type objects
    NominalDiameterOrWidth = [0.015] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = [0.02] (IFCPOSITIVELENGTHMEASURE) [METRE]
    Shape in {"RECTANGULAR"} (IFCTEXT)
  Pset_DuctFittingTypeCommon | properties | on 3 type objects
    NominalDiameterOrWidth = [0.015] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = [0.6] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_DuctFittingTypeCommon | properties | on 2 type objects
    NominalDiameterOrWidth = [0.015] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalHeight = [0.1] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_PipeSegmentTypeCommon | properties | on 1 type object
    InnerDiameter = [0.028] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.032] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.032] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_PipeSegmentTypeCommon | properties | on 1 type object
    InnerDiameter = [0.021] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.025] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.025] (IFCPOSITIVELENGTHMEASURE) [METRE]
  Pset_PipeFittingTypeCommon | properties | on 1 type object
    InnerDiameter = [0.021] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.025] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.025] (IFCPOSITIVELENGTHMEASURE) [METRE]
    SubType = "BEND_90DEGREE" (IFCLABEL)
  Pset_PipeFittingTypeCommon | properties | on 1 type object
    InnerDiameter = [0.028] (IFCPOSITIVELENGTHMEASURE) [METRE]
    NominalDiameter = [0.032] (IFCPOSITIVELENGTHMEASURE) [METRE]
    OuterDiameter = [0.032] (IFCPOSITIVELENGTHMEASURE) [METRE]
    SubType = "BEND_90DEGREE" (IFCLABEL)