NOTE    THIS IS a DATABASE FOR VERSION 1.38 OF 22DISK BY SYDEX.
note
note  Last update: 28.3.1994
note  ----------------------
note  skip = initial tracks in Single Density
note  order sides even-odd = ???;  order eagle !
note  see = ?? (cross reference)


note BEGIN HD1  Hd-TestFormat 3.5"
note DENSITY MFM,HIGH CYLINDERS 80 SIDES 2 SECTORS 18,512
note SIDE1 0 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
note SIDE2 1 1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18
note ORDER SIDES
note BSH 5 BLM 31 EXM 3 DSM 176 DRM 127 AL0 080H AL1 0 OFS 0
note END



BEGIN KCS1  KC Compact 169K System Format
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 0
END

BEGIN KCD1  KC Compact 178K Data Format
DENSITY MFM,LOW CYLINDERS 80 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
BSH 3 BLM 7 EXM 0 DSM 179 DRM 63 AL0 0C0H AL1 0 OFS 0
END

BEGIN P2  Amstrad PCW8256 - DSDD 48 tpi - 9x512x40x2
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS1
BSH 4  BLM 15  EXM 0  DSM 356  DRM 255  AL0 0F0H  AL1 0  OFS 1
END

BEGIN P1  Amstrad PCW8256 - DSDD 96tpi - 9x512x80x2
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9
SIDE2 1 1,2,3,4,5,6,7,8,9
ORDER SIDES LABEL AMS1
BSH 4  BLM 15  EXM 0  DSM 356  DRM 255  AL0 0F0H  AL1 0  OFS 1
END

BEGIN AP2  Amstrad CPC DiskPara 3-Format DSDD 96tpi 10x512x80x2
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 1 1,2,3,4,5,6,7,8,9,10
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 399  DRM 127  AL0 0C0H  AL1 0  OFS 0
END

BEGIN AP1  Amstrad CPC 830K-DiskPara-Format - DDSS 10x512x83x2
DENSITY MFM,LOW CYLINDERS 83 SIDES 2 SECTORS 10,512 SKEW 2
SIDE1 0 1,2,3,4,5,6,7,8,9,10
SIDE2 0 11,12,13,14,15,16,17,18,19,20
ORDER SIDES
BSH 4  BLM 15  EXM 0  DSM 414  DRM 191  AL0 224  AL1 0  OFS 0
END

BEGIN V1  Vortex - DSDD 96 tpi 5.25 - 9x512x80x2
DENSITY MFM,LOW CYLINDERS 80 SIDES 2 SECTORS 9,512
SIDE1 0 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h, 009h
SIDE2 1 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h, 009h
ORDER SIDES
BSH 5 BLM 31 EXM 3 DSM 176 DRM 127 AL0 080H AL1 0 OFS 2
END

BEGIN AI2  Amstrad CPC 154K IBM CP/M-86 SSDD Side 2
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 8,512
SIDE1 0 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h
SIDE2 0 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 41
END

BEGIN AI1  Amstrad CPC 154K IBM CP/M-86 SSDD Side 1
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 8,512
SIDE1 0 001h, 002h, 003h, 004h, 005h, 006h, 007h, 008h
BSH 3 BLM 7 EXM 0 DSM 155 DRM 63 AL0 0C0H AL1 0 OFS 1
END

BEGIN AS2  Amstrad CPC 169K System Side 2
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
SIDE2 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 42
END

BEGIN AS1  Amstrad CPC 169K System Side 1
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 041h, 042h, 043h, 044h, 045h, 046h, 047h, 048h, 049h
BSH 3 BLM 7 EXM 0 DSM 170 DRM 63 AL0 0C0H AL1 0 OFS 2
END

BEGIN AD2  Amstrad CPC 178K Data Side 2
DENSITY MFM,LOW CYLINDERS 40 SIDES 2 SECTORS 9,512 SKEW 2
SIDE1 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
SIDE2 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
ORDER EAGLE
BSH 3 BLM 7 EXM 0 DSM 179 DRM 63 AL0 0C0H AL1 0 OFS 40
END

BEGIN AD1  Amstrad CPC 178K Data Side 1
DENSITY MFM,LOW CYLINDERS 40 SIDES 1 SECTORS 9,512 SKEW 2
SIDE1 0 0c1h, 0c2h, 0c3h, 0c4h, 0c5h, 0c6h, 0c7h, 0c8h, 0c9h
BSH 3 BLM 7 EXM 0 DSM 179 DRM 63 AL0 0c0H AL1 0 OFS 0
END

NOTE End of cpmdisks.def
